{"text_format":"1","workbook":"xlsx","n_sheets":5,"sheets":["Datos","SA","CEV-CEVE","Calculo","Resultados"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":29,"comments":2,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Datos","index":0,"n_rows":388,"n_cols":32,"rows_kept":388,"cut":false,"hidden":true,"merged":[]}
[1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26,27,28,29,30,31,32]
[null,"t correlativo global",3196800,null,null,null,"Mes","T° exterior","Qsol_dif [W/m2]","Qsol_dir [W/m2]","Qgen Pers [W/m2]","Qgen Ilum [W/m2]","Qgen Equip [W/m2]","TsolH","TsolN","TsolNE","TsolE","TsolSE","TsolS","TsolSO","TsolO","TsolNO","Clima [0, 1 o 2]","N [RAH]","G total [W/m2]","TmaxD","TminD","TmaxN","TminN","Tsuelo","Infil RAH","Cat. Mes"]
[null,"h sol",17,null,null,null,{"$f":"+IF(C2<86400*(C11+1),QUOTIENT(C2,C5)+1,QUOTIENT(C2-86400,C5)+1)","v":13},{"$f":"INDIRECT(H36&35+32*($G$3-1))","v":0},{"$f":"INDIRECT(I36&35+32*($G$3-1))","v":0},0,0,{"$f":"INDIRECT(L36&35+32*($G$3-1))","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"INDIRECT(\"E\"&13+32*($G$3-1))","v":0},{"$f":"INDIRECT(\"E\"&15+32*($G$3-1))","v":0},{"$f":"INDIRECT(\"E\"&17+32*($G$3-1))","v":0},{"$f":"INDIRECT(\"E\"&19+32*($G$3-1))","v":0},{"$f":"INDIRECT(\"E\"&21+32*($G$3-1))","v":0},{"$f":"INDIRECT(\"E\"&23+32*($G$3-1))","v":0},{"$f":"INDIRECT(\"E\"&25+32*($G$3-1))","v":0}]
[null,"Columna tiempo","G"]
[null,"t correlativo max mensual",{"$f":"IF(C2<86400*(C11+1),(C11+1)*86400,C11*86400)","v":259200}]
[null,"t residual diario",{"$f":"$C$2-QUOTIENT($C$2,86400)*86400","v":0}]
[null,"Absortividad solar",0.6]
[null,"t residual horario",{"$f":"$C$6-QUOTIENT($C$6,3600)*3600","v":0},null,null,null,null,null,"Rad Ventanas: Sol Incidente*FS*FAV*FAR [W]"]
[null,null,null,null,"Mes","Tiempo [hrs]","Tiempo [s]","T° exterior","Difuso","Directo","Qgen Pers [W/m2]","Qgen Ilum [W/m2]","Qgen Equip [W/m2]","TsolH","TsolN","TsolNE","TsolE","TsolSE","TsolS","TsolSO","TsolO","TsolNO","Clima [0, 1 o 2]","N [RAH]","G total [W/m2]"]
[null,"Fila inicial intervalo",{"$f":"TRUNC($C$6/3600,0)+10+32*(E11-1)","v":10},null,"Enero",0,0,14.437182795698925,0,0,4.0999999999999996,0,0,14.437182795698925,14.437182795698925,14.437182795698925,14.437182795698925,14.437182795698925,14.437182795698925,14.437182795698925,14.437182795698925,14.437182795698925,0,0.82620000000000016,0]
[null,"dias por mes",3,null,1,1,3600,13.426860215053761,0,0,4.0999999999999996,0,0,13.426860215053761,13.426860215053761,13.426860215053761,13.426860215053761,13.426860215053761,13.426860215053761,13.426860215053761,13.426860215053761,13.426860215053761,0,0.82620000000000016,0]
[null,null,null,null,"Tmax Dia",2,7200,12.882408602150537,0,0,4.0999999999999996,0,0,12.882408602150537,12.882408602150537,12.882408602150537,12.882408602150537,12.882408602150537,12.882408602150537,12.882408602150537,12.882408602150537,12.882408602150537,0,0.82620000000000016,0]
[null,null,null,null,26.337677419354836,3,10800,12.360408602150539,0,0,4.0999999999999996,0,0,12.360408602150539,12.360408602150539,12.360408602150539,12.360408602150539,12.360408602150539,12.360408602150539,12.360408602150539,12.360408602150539,12.360408602150539,0,0.82620000000000016,0]
[null,null,null,null,"Tmin Dia",4,14400,11.956279569892475,0,0,4.0999999999999996,0,0,11.956279569892475,11.956279569892475,11.956279569892475,11.956279569892475,11.956279569892475,11.956279569892475,11.956279569892475,11.956279569892475,11.956279569892475,0,0.82620000000000016,0]
[null,null,null,null,21.337677419354836,5,18000,12.180795698924733,0,0,4.0999999999999996,0,0,12.180795698924733,12.180795698924733,12.180795698924733,12.180795698924733,12.180795698924733,12.180795698924733,12.180795698924733,12.180795698924733,12.180795698924733,0,0.82620000000000016,0]
[null,null,null,null,"Tmax Noche",6,21600,14.347376344086017,216.65754453850744,0,3.28,0,0,14.347376344086017,14.347376344086017,14.347376344086017,14.347376344086017,14.347376344086017,14.347376344086017,14.347376344086017,14.347376344086017,14.347376344086017,0,0.82620000000000016,12.451612903225806]
[null,null,null,null,26.337677419354836,7,25200,16.732860215053762,1894.3502922732193,315.76027034842298,3.9359999999999999,0,0,16.732860215053762,16.732860215053762,16.732860215053762,16.732860215053762,16.732860215053762,16.732860215053762,16.732860215053762,16.732860215053762,16.732860215053762,0,0.82620000000000016,191.29032258064515]
[null,null,null,null,"Tmin Noche",8,28800,19.219376344086026,2348.9943624187918,1007.3432342896267,1.968,0,0,19.219376344086026,19.219376344086026,19.219376344086026,19.219376344086026,19.219376344086026,19.219376344086026,19.219376344086026,19.219376344086026,19.219376344086026,0,3.8262,397.93548387096774]
[null,null,null,null,19.337677419354836,9,32400,21.47015053763441,3198.7858713081705,1622.5505242287459,1.23,0,0,21.47015053763441,21.47015053763441,21.47015053763441,21.47015053763441,21.47015053763441,21.47015053763441,21.47015053763441,21.47015053763441,21.47015053763441,0,3.8262,607.35483870967744]
[null,null,null,null,"Tsuelo",10,36000,23.468344086021503,4095.1643651630834,2052.0092089492041,1.23,0,0,23.468344086021503,23.468344086021503,23.468344086021503,23.468344086021503,23.468344086021503,23.468344086021503,23.468344086021503,23.468344086021503,23.468344086021503,0,3.8262,770.9677419354839]
[null,null,null,null,19.363440860215054,11,39600,24.843505376344087,4921.3817370819506,2330.9410798597291,1.23,0,0,24.843505376344087,24.843505376344087,24.843505376344087,24.843505376344087,24.843505376344087,24.843505376344087,24.843505376344087,24.843505376344087,24.843505376344087,0,3.8262,891.25806451612902]
[null,null,null,null,"Infil RAH",12,43200,25.898731182795704,5988.3920794853266,887.47572957779846,1.23,0,0,25.898731182795704,25.898731182795704,25.898731182795704,25.898731182795704,25.898731182795704,25.898731182795704,25.898731182795704,25.898731182795704,25.898731182795704,0,0.82620000000000016,876.83870967741939]
[null,null,null,null,0,13,46800,26.493698924731184,6101.7724525339745,2125.238443615704,1.23,0,0,26.493698924731184,26.493698924731184,26.493698924731184,26.493698924731184,26.493698924731184,26.493698924731184,26.493698924731184,26.493698924731184,26.493698924731184,0,0.82620000000000016,883.51612903225805]
[null,null,null,null,"Cat Mes",14,50400,26.639634408602152,5404.6515449774306,2028.8706270357206,1.23,0,0,26.639634408602152,26.639634408602152,26.639634408602152,26.639634408602152,26.639634408602152,26.639634408602152,26.639634408602152,26.639634408602152,26.639634408602152,0,3.8262,819.29032258064512]
[null,null,null,null,"v",15,54000,26.297247311827952,4641.8598272887475,1757.1365434350209,1.23,0,0,26.297247311827952,26.297247311827952,26.297247311827952,26.297247311827952,26.297247311827952,26.297247311827952,26.297247311827952,26.297247311827952,26.297247311827952,0,3.8262,707.32258064516134]
[null,null,null,null,null,16,57600,25.382344086021504,3603.4752226352789,1360.3430236317251,1.476,0,0,25.382344086021504,25.382344086021504,25.382344086021504,25.382344086021504,25.382344086021504,25.382344086021504,25.382344086021504,25.382344086021504,25.382344086021504,0,3.8262,548.16129032258061]
[null,null,null,null,null,17,61200,23.934215053763435,2552.1809715455788,894.97267307124571,2.46,0,0,23.934215053763435,23.934215053763435,23.934215053763435,23.934215053763435,23.934215053763435,23.934215053763435,23.934215053763435,23.934215053763435,23.934215053763435,0,3.8262,371.06451612903226]
[null,null,null,null,null,18,64800,22.177376344086017,1873.5826001801497,289.36077368275329,2.46,0,0,22.177376344086017,22.177376344086017,22.177376344086017,22.177376344086017,22.177376344086017,22.177376344086017,22.177376344086017,22.177376344086017,22.177376344086017,0,0.82620000000000016,180.2258064516129]
[null,null,null,null,null,19,68400,20.824666666666662,226.19945712180959,0,3.69,0,0,20.824666666666662,20.824666666666662,20.824666666666662,20.824666666666662,20.824666666666662,20.824666666666662,20.824666666666662,20.824666666666662,20.824666666666662,0,0.82620000000000016,13]
[null,null,null,null,null,20,72000,19.4663440860215,0,0,4.4279999999999999,1.5,0,19.4663440860215,19.4663440860215,19.4663440860215,19.4663440860215,19.4663440860215,19.4663440860215,19.4663440860215,19.4663440860215,19.4663440860215,0,0.82620000000000016,0]
[null,null,null,null,null,21,75600,18.113634408602152,0,0,4.92,1.5,0,18.113634408602152,18.113634408602152,18.113634408602152,18.113634408602152,18.113634408602152,18.113634408602152,18.113634408602152,18.113634408602152,18.113634408602152,0,3.8262,0]
[null,null,null,null,null,22,79200,16.766537634408596,0,0,4.0999999999999996,0,0,16.766537634408596,16.766537634408596,16.766537634408596,16.766537634408596,16.766537634408596,16.766537634408596,16.766537634408596,16.766537634408596,16.766537634408596,0,3.8262,0]
[null,null,null,null,null,23,82800,15.40260215053763,0,0,4.0999999999999996,0,0,15.40260215053763,15.40260215053763,15.40260215053763,15.40260215053763,15.40260215053763,15.40260215053763,15.40260215053763,15.40260215053763,15.40260215053763,0,0.82620000000000016,0]
[null,null,null,null,null,24,86400,14.437182795698925,0,0,4.0999999999999996,0,0,14.437182795698925,14.437182795698925,14.437182795698925,14.437182795698925,14.437182795698925,14.437182795698925,14.437182795698925,14.437182795698925,14.437182795698925,0,0.82620000000000016,0]
[null,null,null,null,null,null,"Valor Variable",{"$f":"+INDIRECT(H36&$C10)+((INDIRECT(H36&$C10+1)-INDIRECT(H36&$C10))/(INDIRECT($C$4&$C10+1)-INDIRECT($C$4&$C10)))*($C$6-INDIRECT($C$4&$C10))","v":14.437182795698925},{"$f":"+INDIRECT(I36&$C10)+((INDIRECT(I36&$C10+1)-INDIRECT(I36&$C10))/(INDIRECT($C$4&$C10+1)-INDIRECT($C$4&$C10)))*($C$6-INDIRECT($C$4&$C10))","v":0},0,4.0999999999999996,0,{"$f":"+INDIRECT(M36&$C10)+((INDIRECT(M36&$C10+1)-INDIRECT(M36&$C10))/(INDIRECT($C$4&$C10+1)-INDIRECT($C$4&$C10)))*($C$6-INDIRECT($C$4&$C10))","v":0},{"$f":"+INDIRECT(N36&$C10)+((INDIRECT(N36&$C10+1)-INDIRECT(N36&$C10))/(INDIRECT($C$4&$C10+1)-INDIRECT($C$4&$C10)))*($C$6-INDIRECT($C$4&$C10))","v":14.437182795698925},14.437182795698925,14.437182795698925,14.437182795698925,14.437182795698925,14.437182795698925,14.437182795698925,14.437182795698925,14.437182795698925,{"$f":"+INDIRECT(W36&$C10)","v":0},0.82620000000000016,0]
[null,null,null,null,null,null,null,{"$f":"MID(ADDRESS(ROW(),COLUMN()),2,1)","v":"H"},{"$f":"MID(ADDRESS(ROW(),COLUMN()),2,1)","v":"I"},"J","K","L","M","N","O","P","Q","R","S","T","U","V","W","X","Y"]
[null,null,null,null,null,null,"Aext",{"$f":"+MAX(H10:H33)-MIN(H10:H33)","v":14.683354838709677},"°C"]
[null,null,null,null,null,null,"Text_media",{"$f":"+AVERAGE(H10:H33)","v":19.363440860215054},"°C"]
[null,null,null,null,null,null,"Sol Peak",{"$f":"+MAX(I10:I34)","v":6101.7724525339745}]
[null,null,null,null,null,null,null,null,"Rad Ventanas: Sol Incidente*FS*FAV*FAR [W]"]
[null,null,null,null,"Mes","Tiempo [hrs]","Tiempo [s]","T° exterior","Difuso","Directo","Qgen Pers [W/m2]","Qgen Ilum [W/m2]","Qgen Equip [W/m2]","TsolH","TsolN","TsolNE","TsolE","TsolSE","TsolS","TsolSO","TsolO","TsolNO","Clima [0, 1 o 2]","N [RAH]","G total [W/m2]"]
[null,"Fila inicial intervalo",{"$f":"TRUNC($C$6/3600,0)+10+32*(E43-1)","v":42},null,"Febrero",0,0,14.090178571428572,0,0,4.0999999999999996,0,0,10.384296218487396,14.090178571428572,14.090178571428572,14.090178571428572,14.090178571428572,14.090178571428572,14.090178571428572,14.090178571428572,14.090178571428572,0,0.82620000000000016,0]
[null,null,null,null,2,1,3600,13.065178571428573,0,0,4.0999999999999996,0,0,9.3592962184873976,13.065178571428573,13.065178571428573,13.065178571428573,13.065178571428573,13.065178571428573,13.065178571428573,13.065178571428573,13.065178571428573,0,0.82620000000000016,0]
[null,null,null,null,"Tmax Dia",2,7200,12.508928571428573,0,0,4.0999999999999996,0,0,8.8030462184873954,12.508928571428573,12.508928571428573,12.508928571428573,12.508928571428573,12.508928571428573,12.508928571428573,12.508928571428573,12.508928571428573,0,0.82620000000000016,0]
[null,null,null,null,26.207964285714283,3,10800,11.971428571428572,0,0,4.0999999999999996,0,0,8.265546218487394,11.971428571428572,11.971428571428572,11.971428571428572,11.971428571428572,11.971428571428572,11.971428571428572,11.971428571428572,11.971428571428572,0,0.82620000000000016,0]
[null,null,null,null,"Tmin Dia",4,14400,11.596428571428572,0,0,4.0999999999999996,0,0,7.8905462184873949,11.596428571428572,11.596428571428572,11.596428571428572,11.596428571428572,11.596428571428572,11.596428571428572,11.596428571428572,11.596428571428572,0,0.82620000000000016,0]
[null,null,null,null,21.207964285714283,5,18000,11.602678571428571,0,0,4.0999999999999996,0,0,7.8967962184873945,11.602678571428571,11.602678571428571,11.602678571428571,11.602678571428571,11.602678571428571,11.602678571428571,11.602678571428571,11.602678571428571,0,0.82620000000000016,0]
[null,null,null,null,"Tmax Noche",6,21600,13.408928571428572,70.842687120566737,0,3.28,0,0,9.8706932773109237,13.462463416109271,13.491634136892678,13.506072710975346,13.490563062975674,13.460948688849541,13.490563062975674,13.506072710975346,13.491634136892678,0,0.82620000000000016,4.0714285714285712]
[null,null,null,null,26.207964285714283,7,25200,15.80892857142857,1481.4821587318515,189.58320077695765,3.9359999999999999,0,0,18.020693277310922,17.698614667877127,18.728289934828279,19.237946269114705,18.690482904635097,17.645147453024876,18.690482904635097,19.237946269114705,18.728289934828279,0,0.82620000000000016,143.71428571428572]
[null,null,null,null,"Tmin Noche",8,28800,18.346428571428568,2278.7731023782303,710.12780632490876,1.968,0,0,29.067016806722688,22.953242837372983,25.463460125839887,26.705937421900977,25.371291396666152,22.822896570548792,25.371291396666152,26.705937421900977,25.463460125839887,0,0.82620000000000016,350.35714285714283]
[null,null,null,null,19.207964285714283,9,32400,20.690178571428568,3373.7276173469895,1184.0606199936637,1.23,0,0,39.862237394957987,27.995806454741238,31.976586307613779,33.946945053263356,31.830422299483722,27.789099332112901,31.830422299483722,33.946945053263356,31.976586307613779,0,0.82620000000000016,555.60714285714289]
[null,null,null,null,"Tsuelo",10,36000,22.721428571428568,4304.0039561144313,1528.1256283508269,1.23,0,0,48.422899159663864,32.112097773884273,37.229000436215841,39.761703646137718,37.041120917634068,31.846396010613795,37.041120917634068,39.761703646137718,37.229000436215841,0,3.8262,714.17857142857144]
[null,null,null,null,18.854761904761904,11,39600,24.283928571428568,5316.9300965225348,1695.1894737271052,1.23,0,0,54.483928571428571,35.111116106149716,41.010766442836051,43.930904723976155,40.794146440814671,34.804769161409794,40.794146440814671,43.930904723976155,41.010766442836051,0,3.8262,823.42857142857144]
[null,null,null,null,"Infil RAH",12,43200,25.471428571428568,5917.2286558073365,664.81767870748126,1.23,0,0,56.883193277310923,36.685569720333021,42.79606807390995,45.82056938175284,42.571706274453391,36.368274220663118,42.571706274453391,45.82056938175284,42.79606807390995,0,3.8262,852.85714285714289]
[null,null,null,null,0,13,46800,26.133928571428573,6039.6497905683163,1889.1782101635085,1.23,0,0,58.038340336134453,37.505387027070171,43.701606358387806,46.768536809368364,43.474097104876897,37.183640355189652,43.474097104876897,46.768536809368364,43.701606358387806,0,3.8262,864.82142857142856]
[null,null,null,null,"Cat Mes",14,50400,26.365178571428576,5485.3368352038824,1737.4809532215709,1.23,0,0,55.246060924369758,36.771131407214746,42.441254230368479,45.247783731226548,42.233061888904579,36.476702974334287,42.233061888904579,45.247783731226548,42.441254230368479,0,0.82620000000000016,791.39285714285711]
[null,null,null,null,"v",15,54000,26.040178571428566,4555.0604964364402,1548.1200302519533,1.23,0,0,50.582825630252103,35.060799900126455,39.976066352130616,42.408966085060015,39.79559039711549,34.805568356861833,39.79559039711549,42.408966085060015,39.976066352130616,0,3.8262,686.03571428571433]
[null,null,null,null,null,16,57600,25.027678571428577,3461.9702627076954,1142.0319075797925,1.476,0,0,42.532090336134459,31.800775631338496,35.491383577470828,37.318116507245449,35.355873936199387,31.609136058820113,35.355873936199387,37.318116507245449,35.491383577470828,0,3.8262,515.10714285714289]
[null,null,null,null,null,17,61200,23.477678571428573,2281.2588106982503,693.06319560761915,2.46,0,0,33.070325630252107,27.724306645530035,30.038261277498052,31.183594833897686,29.953298808800994,27.604151570005961,29.953298808800994,31.183594833897686,30.038261277498052,0,3.8262,322.96428571428572]
[null,null,null,null,null,18,64800,21.71517857142857,1396.9680758511756,176.49114884423358,2.46,0,0,23.326943277310921,23.413266276388306,24.33854106895674,24.796522506526248,24.3045673559402,23.365220190676148,24.3045673559402,24.796522506526248,24.33854106895674,0,3.8262,129.14285714285714]
[null,null,null,null,null,19,68400,20.358928571428571,50.335593480402679,0,3.69,0,0,16.772163865546215,20.39696648738591,20.417693052153069,20.42795203900128,20.416932025948881,20.395890233806629,20.416932025948881,20.42795203900128,20.417693052153069,0,0.82620000000000016,2.8928571428571428]
[null,null,null,null,null,20,72000,19.002678571428579,0,0,4.4279999999999999,1.5,0,15.296796218487401,19.002678571428579,19.002678571428579,19.002678571428579,19.002678571428579,19.002678571428579,19.002678571428579,19.002678571428579,19.002678571428579,0,0.82620000000000016,0]
[null,null,null,null,null,21,75600,17.640178571428567,0,0,4.92,1.5,0,13.93429621848739,17.640178571428567,17.640178571428567,17.640178571428567,17.640178571428567,17.640178571428567,17.640178571428567,17.640178571428567,17.640178571428567,0,0.82620000000000016,0]
[null,null,null,null,null,22,79200,16.277678571428574,0,0,4.0999999999999996,0,0,12.571796218487396,16.277678571428574,16.277678571428574,16.277678571428574,16.277678571428574,16.277678571428574,16.277678571428574,16.277678571428574,16.277678571428574,0,3.8262,0]
[null,null,null,null,null,23,82800,14.908928571428572,0,0,4.0999999999999996,0,0,11.203046218487394,14.908928571428572,14.908928571428572,14.908928571428572,14.908928571428572,14.908928571428572,14.908928571428572,14.908928571428572,14.908928571428572,0,0.82620000000000016,0]
[null,null,null,null,null,24,86400,14.090178571428572,0,0,4.0999999999999996,0,0,10.384296218487396,14.090178571428572,14.090178571428572,14.090178571428572,14.090178571428572,14.090178571428572,14.090178571428572,14.090178571428572,14.090178571428572,0,0.82620000000000016,0]
[null,null,null,null,null,null,"Valor Variable",{"$f":"+INDIRECT(H68&$C42)+((INDIRECT(H68&$C42+1)-INDIRECT(H68&$C42))/(INDIRECT($C$4&$C42+1)-INDIRECT($C$4&$C42)))*($C$6-INDIRECT($C$4&$C42))","v":14.090178571428572},{"$f":"+INDIRECT(I68&$C42)+((INDIRECT(I68&$C42+1)-INDIRECT(I68&$C42))/(INDIRECT($C$4&$C42+1)-INDIRECT($C$4&$C42)))*($C$6-INDIRECT($C$4&$C42))","v":0},0,4.0999999999999996,0,{"$f":"+INDIRECT(M68&$C42)+((INDIRECT(M68&$C42+1)-INDIRECT(M68&$C42))/(INDIRECT($C$4&$C42+1)-INDIRECT($C$4&$C42)))*($C$6-INDIRECT($C$4&$C42))","v":0},10.384296218487396,14.090178571428572,14.090178571428572,14.090178571428572,14.090178571428572,14.090178571428572,14.090178571428572,14.090178571428572,14.090178571428572,{"$f":"+INDIRECT(W68&$C42)","v":0},0.82620000000000016,0]
[null,null,null,null,null,null,null,{"$f":"MID(ADDRESS(ROW(),COLUMN()),2,1)","v":"H"},{"$f":"MID(ADDRESS(ROW(),COLUMN()),2,1)","v":"I"},"J","K","L","M","N","O","P","Q","R","S","T","U","V","W","X","Y"]
[]
[]
[]
[null,null,null,null,null,null,null,null,"Rad Ventanas: Sol Incidente*FS*FAV*FAR [W]"]
[null,null,null,null,"Mes","Tiempo [hrs]","Tiempo [s]","T° exterior","Difuso","Directo","Qgen Pers [W/m2]","Qgen Ilum [W/m2]","Qgen Equip [W/m2]","TsolH","TsolN","TsolNE","TsolE","TsolSE","TsolS","TsolSO","TsolO","TsolNO","Clima [0, 1 o 2]","N [RAH]","G total [W/m2]"]
[null,"Fila inicial intervalo",{"$f":"TRUNC($C$6/3600,0)+10+32*(E75-1)","v":74},null,"Marzo",0,0,13.068911290322582,0,0,4.0999999999999996,0,0,9.3630289373814044,13.068911290322582,13.068911290322582,13.068911290322582,13.068911290322582,13.068911290322582,13.068911290322582,13.068911290322582,13.068911290322582,0,0.82620000000000016,0]
[null,null,null,null,3,1,3600,12.081040322580646,0,0,4.0999999999999996,0,0,8.3751579696394707,12.081040322580646,12.081040322580646,12.081040322580646,12.081040322580646,12.081040322580646,12.081040322580646,12.081040322580646,12.081040322580646,0,0.82620000000000016,0]
[null,null,null,null,"Tmax Dia",2,7200,11.390653225806453,0,0,4.0999999999999996,0,0,7.6847708728652764,11.390653225806453,11.390653225806453,11.390653225806453,11.390653225806453,11.390653225806453,11.390653225806453,11.390653225806453,11.390653225806453,0,0.82620000000000016,0]
[null,null,null,null,25.826614919354839,3,10800,10.891104838709678,0,0,4.0999999999999996,0,0,7.1852224857685014,10.891104838709678,10.891104838709678,10.891104838709678,10.891104838709678,10.891104838709678,10.891104838709678,10.891104838709678,10.891104838709678,0,0.82620000000000016,0]
[null,null,null,null,"Tmin Dia",4,14400,10.464524193548387,0,0,4.0999999999999996,0,0,6.7586418406072104,10.464524193548387,10.464524193548387,10.464524193548387,10.464524193548387,10.464524193548387,10.464524193548387,10.464524193548387,10.464524193548387,0,0.82620000000000016,0]
[null,null,null,null,20.826614919354839,5,18000,10.318588709677421,0,0,4.0999999999999996,0,0,6.6127063567362443,10.318588709677421,10.318588709677421,10.318588709677421,10.318588709677421,10.318588709677421,10.318588709677421,10.318588709677421,10.318588709677421,0,0.82620000000000016,0]
[null,null,null,null,"Tmax Noche",6,21600,11.40749193548387,2.2451559019534448,0,3.28,0,0,7.7069226755218212,11.410041562381108,11.410595869928384,11.410628814951215,11.409774468169566,11.408879924873631,11.409774468169566,11.410628814951215,11.410595869928384,0,0.82620000000000016,0.12903225806451613]
[null,null,null,null,25.826614919354839,7,25200,13.882782258064518,703.29508628691667,100.76937272654897,3.9359999999999999,0,0,12.964945445920304,15.220698972390503,15.511571857822823,15.52885975855404,15.080541284883191,14.611129690341834,15.080541284883191,15.52885975855404,15.511571857822821,0,0.82620000000000016,67.709677419354833]
[null,null,null,null,"Tmin Noche",8,28800,16.655556451612906,1823.0665923861973,588.29779183974642,1.968,0,0,23.824247153700192,21.874005303536126,23.008534275920308,23.075964501402197,21.327330226060013,19.496423735107129,21.327330226060013,23.075964501402197,23.008534275920304,0,0.82620000000000016,264.09677419354841]
[null,null,null,null,18.826614919354839,9,32400,19.097169354838712,2263.6784381445609,1274.1489125956202,1.23,0,0,34.956751897533209,28.486170403920063,30.527407946758586,30.648727993338312,27.502595969912107,24.208440282635209,27.502595969912107,30.648727993338312,30.527407946758583,0,0.82620000000000016,475.16129032258067]
[null,null,null,null,"Tsuelo",10,36000,21.353556451612899,3224.6051641806348,1616.4789093049603,1.23,0,0,43.304600094876662,33.665704738378373,36.342455884167165,36.501547399424055,32.375906790836098,28.056157214770884,32.375906790836098,36.501547399424055,36.342455884167158,0,3.8262,623.09677419354841]
[null,null,null,null,17.359274193548391,11,39600,22.796072580645163,4414.5377922159614,1853.7514748738558,1.23,0,0,50.208975806451619,37.729237317771975,40.975816622159002,41.16877562088743,36.164866520763255,30.925526436477906,36.164866520763255,41.16877562088743,40.975816622158995,0,3.8262,755.74193548387098]
[null,null,null,null,"Infil RAH",12,43200,23.88497580645161,4968.5300110229737,857.87933618113368,1.23,0,0,50.067898007590131,38.227901916867673,41.34615902406064,41.531491250003413,36.725363429831219,31.693110118554582,36.725363429831219,41.531491250003413,41.346159024060633,0,3.8262,725.87096774193549]
[null,null,null,null,0,13,46800,24.536072580645161,5243.5616090122712,1884.6176744706891,1.23,0,0,51.097552656546497,39.060659607489477,42.218411127425753,42.406090686245321,37.539090657880564,32.443101136768632,37.539090657880564,42.406090686245321,42.218411127425753,0,3.8262,735.06451612903231]
[null,null,null,null,"Cat Mes",14,50400,24.693233870967742,4787.2336719402329,1798.551831992072,1.23,0,0,49.359268026565466,38.308241502222167,41.268243804668245,41.444170226592419,36.881958412581305,32.105097212293821,36.881958412581305,41.444170226592419,41.268243804668245,0,3.8262,689.0322580645161]
[null,null,null,null,"v",15,54000,24.232975806451602,3747.1652003602994,1611.8422193185907,1.23,0,0,44.668459677419349,35.817843020779748,38.33647793870847,38.486171886202463,34.604233697080183,30.539652596180137,34.604233697080183,38.486171886202463,38.33647793870847,0,3.8262,586.29032258064512]
[null,null,null,null,null,16,57600,23.132846774193549,2703.1677059519475,1220.7612738538664,1.476,0,0,37.391860056925999,31.753772720481756,33.628025114703817,33.739420473155334,30.850660417701199,27.825985898324411,30.850660417701199,33.739420473155334,33.628025114703817,0,3.8262,436.29032258064518]
[null,null,null,null,null,17,61200,21.437750000000008,1998.1887527385661,606.52589642504063,2.46,0,0,28.207958728652759,26.464976834630328,27.557932740968919,27.622892089738389,25.93833382301996,24.174518079262125,25.93833382301996,27.622892089738389,27.557932740968916,0,3.8262,254.41935483870967]
[null,null,null,null,null,18,64800,19.944717741935481,723.50148940449753,86.441963428955603,2.46,0,0,18.980391366223905,21.260325220910627,21.546347915304295,21.56334754708573,21.122504607754319,20.660920267052383,21.122504607754319,21.56334754708573,21.546347915304295,0,0.82620000000000016,66.58064516129032]
[null,null,null,null,null,19,68400,18.737943548387101,3.9290228284185282,0,3.69,1.5,0,15.041359108159394,18.742405395457268,18.743375433664998,18.743433087454957,18.741937980587068,18.740372529819183,18.741937980587068,18.743433087454957,18.743375433664998,0,0.82620000000000016,0.22580645161290322]
[null,null,null,null,null,20,72000,17.497491935483868,0,0,4.4279999999999999,1.5,0,13.791609582542691,17.497491935483868,17.497491935483868,17.497491935483868,17.497491935483868,17.497491935483868,17.497491935483868,17.497491935483868,17.497491935483868,0,0.82620000000000016,0]
[null,null,null,null,null,21,75600,16.285104838709678,0,0,4.92,1.5,0,12.579222485768501,16.285104838709678,16.285104838709678,16.285104838709678,16.285104838709678,16.285104838709678,16.285104838709678,16.285104838709678,16.285104838709678,0,0.82620000000000016,0]
[null,null,null,null,null,22,79200,15.039040322580645,0,0,4.0999999999999996,0,0,11.333157969639469,15.039040322580645,15.039040322580645,15.039040322580645,15.039040322580645,15.039040322580645,15.039040322580645,15.039040322580645,15.039040322580645,0,3.8262,0]
[null,null,null,null,null,23,82800,13.792975806451613,0,0,4.0999999999999996,0,0,10.087093453510438,13.792975806451613,13.792975806451613,13.792975806451613,13.792975806451613,13.792975806451613,13.792975806451613,13.792975806451613,13.792975806451613,0,0.82620000000000016,0]
[null,null,null,null,null,24,86400,13.068911290322582,0,0,4.0999999999999996,0,0,9.3630289373814044,13.068911290322582,13.068911290322582,13.068911290322582,13.068911290322582,13.068911290322582,13.068911290322582,13.068911290322582,13.068911290322582,0,0.82620000000000016,0]
[null,null,null,null,null,null,"Valor Variable",{"$f":"+INDIRECT(H100&$C74)+((INDIRECT(H100&$C74+1)-INDIRECT(H100&$C74))/(INDIRECT($C$4&$C74+1)-INDIRECT($C$4&$C74)))*($C$6-INDIRECT($C$4&$C74))","v":13.068911290322582},{"$f":"+INDIRECT(I100&$C74)+((INDIRECT(I100&$C74+1)-INDIRECT(I100&$C74))/(INDIRECT($C$4&$C74+1)-INDIRECT($C$4&$C74)))*($C$6-INDIRECT($C$4&$C74))","v":0},0,4.0999999999999996,0,{"$f":"+INDIRECT(M100&$C74)+((INDIRECT(M100&$C74+1)-INDIRECT(M100&$C74))/(INDIRECT($C$4&$C74+1)-INDIRECT($C$4&$C74)))*($C$6-INDIRECT($C$4&$C74))","v":0},9.3630289373814044,13.068911290322582,13.068911290322582,13.068911290322582,13.068911290322582,13.068911290322582,13.068911290322582,13.068911290322582,13.068911290322582,{"$f":"+INDIRECT(W100&$C74)","v":0},0.82620000000000016,0]
[null,null,null,null,null,null,null,{"$f":"MID(ADDRESS(ROW(),COLUMN()),2,1)","v":"H"},{"$f":"MID(ADDRESS(ROW(),COLUMN()),2,1)","v":"I"},"J","K","L","M","N","O","P","Q","R","S","T","U","V","W","X","Y"]
[]
[]
[]
[null,null,null,null,null,null,null,null,"Rad Ventanas: Sol Incidente*FS*FAV*FAR [W]"]
[null,null,null,null,"Mes","Tiempo [hrs]","Tiempo [s]","T° exterior","Difuso","Directo","Qgen Pers [W/m2]","Qgen Ilum [W/m2]","Qgen Equip [W/m2]","TsolH","TsolN","TsolNE","TsolE","TsolSE","TsolS","TsolSO","TsolO","TsolNO","Clima [0, 1 o 2]","N [RAH]","G total [W/m2]"]
[null,"Fila inicial intervalo",{"$f":"TRUNC($C$6/3600,0)+10+32*(E107-1)","v":106},null,"Abril",0,0,11.6928125,0,0,4.0999999999999996,0,0,7.9869301470588239,11.6928125,11.6928125,11.6928125,11.6928125,11.6928125,11.6928125,11.6928125,11.6928125,0,0.82620000000000016,0]
[null,null,null,null,4,1,3600,10.757812500000002,0,0,4.0999999999999996,0,0,7.0519301470588251,10.757812500000002,10.757812500000002,10.757812500000002,10.757812500000002,10.757812500000002,10.757812500000002,10.757812500000002,10.757812500000002,0,0.82620000000000016,0]
[null,null,null,null,"Tmax Dia",2,7200,9.8228124999999995,0,0,4.0999999999999996,0,0,6.1169301470588229,9.8228124999999995,9.8228124999999995,9.8228124999999995,9.8228124999999995,9.8228124999999995,9.8228124999999995,9.8228124999999995,9.8228124999999995,0,0.82620000000000016,0]
[null,null,null,null,25.273131249999999,3,10800,9.3388124999999995,0,0,4.0999999999999996,0,0,5.6329301470588229,9.3388124999999995,9.3388124999999995,9.3388124999999995,9.3388124999999995,9.3388124999999995,9.3388124999999995,9.3388124999999995,9.3388124999999995,0,0.82620000000000016,0]
[null,null,null,null,"Tmin Dia",4,14400,8.8383125000000007,0,0,4.0999999999999996,0,0,5.1324301470588241,8.8383125000000007,8.8383125000000007,8.8383125000000007,8.8383125000000007,8.8383125000000007,8.8383125000000007,8.8383125000000007,8.8383125000000007,0,0.82620000000000016,0]
[null,null,null,null,20.273131249999999,5,18000,8.5193124999999981,0,0,4.0999999999999996,0,0,4.8134301470588214,8.5193124999999981,8.5193124999999981,8.5193124999999981,8.5193124999999981,8.5193124999999981,8.5193124999999981,8.5193124999999981,8.5193124999999981,0,0.82620000000000016,0]
[null,null,null,null,"Tmax Noche",6,21600,8.805312500000003,0,0,3.28,0,0,5.0994301470588264,8.805312500000003,8.805312500000003,8.805312500000003,8.805312500000003,8.805312500000003,8.805312500000003,8.805312500000003,8.805312500000003,0,0.82620000000000016,0]
[null,null,null,null,25.273131249999999,7,25200,11.3133125,171.67958796937342,0,3.9359999999999999,0,0,8.0137046568627461,11.615910173135722,11.604458055185789,11.559065121138392,11.464004270095668,11.417278525374636,11.464004270095668,11.559065121138392,11.604458055185789,0,0.82620000000000016,9.8666666666666671]
[null,null,null,null,"Tmin Noche",8,28800,13.947812500000001,1664.5960049733167,287.4933163897939,1.968,0,0,16.794479166666665,18.828222268749784,18.643518177219455,17.911403761198237,16.378226386610539,15.624615895738224,16.378226386610539,17.911403761198237,18.643518177219455,0,0.82620000000000016,159.13333333333333]
[null,null,null,null,18.273131249999999,9,32400,16.422812499999999,2336.8143916506942,828.80820045356029,1.23,0,0,25.780851715686271,26.152963354411487,25.784715858980881,24.325087662145961,21.268367458684349,19.765882194310098,21.268367458684349,24.325087662145961,25.784715858980881,0,0.82620000000000016,317.26666666666665]
[null,null,null,null,"Tsuelo",10,36000,18.562312500000008,3163.3124080573061,1228.339353377612,1.23,0,0,33.507998774509815,32.454203649463935,31.928450842634096,29.844516448140528,25.480388391317682,23.335266279783568,25.480388391317682,29.844516448140528,31.928450842634096,0,0.82620000000000016,452.96666666666664]
[null,null,null,null,15.188750000000001,11,39600,20.388312499999998,3789.7109047023177,1522.9294060438351,1.23,0,0,39.494194852941177,37.37876293079627,36.735741983742628,34.186990078783978,28.849451753344599,26.225864330156945,28.849451753344599,34.186990078783978,36.735741983742628,0,3.8262,554]
[null,null,null,null,"Infil RAH",12,43200,21.664312500000001,4314.6096449465167,1152.6221387887433,1.23,0,0,43.863920343137259,40.959003320147346,40.228776042488469,37.334363078939155,31.272949218870398,28.293551563921916,31.272949218870398,37.334363078939155,40.228776042488469,0,3.8262,629.13333333333333]
[null,null,null,null,0,13,46800,22.329812499999999,4438.7293470595096,2041.4073676906005,1.23,0,0,44.467655637254907,41.578500295515227,40.850014049301436,37.962502038563386,31.915539997065309,28.943245918172391,31.915539997065309,37.962502038563386,40.850014049301436,0,3.8262,627.63333333333333]
[null,null,null,null,"Cat Mes",14,50400,22.384812499999999,3981.1104453438488,1789.7019853822928,1.23,0,0,41.548341911764709,39.418199087119582,38.773553177383846,36.218360383134694,30.867333693696011,28.237116266189833,30.867333693696011,36.218360383134694,38.773553177383846,0,3.8262,555.4]
[null,null,null,null,"v",15,54000,21.713812499999996,3104.1525500408329,1471.5083888793376,1.23,0,0,36.411067401960779,35.420669261499178,34.901919270037368,32.845742041295757,28.539742410279445,26.423192460213254,28.539742410279445,32.845742041295757,34.901919270037368,0,3.8262,446.93333333333334]
[null,null,null,null,null,16,57600,20.322312500000006,2147.7348454411817,986.91159696065824,1.476,0,0,29.114861519607853,29.63128010666853,29.278972721357427,27.882526581372261,24.95812080571336,23.520672726558921,24.95812080571336,27.882526581372261,29.278972721357427,0,3.8262,303.53333333333336]
[null,null,null,null,null,17,61200,18.490812500000008,1600.7961580928063,332.9890507605553,2.46,0,0,21.075322303921578,23.17596498642235,22.998650606136739,22.29582690093665,20.823989467393407,20.100529710445812,20.823989467393407,22.29582690093665,22.998650606136739,0,0.82620000000000016,152.76666666666668]
[null,null,null,null,null,18,64800,17.456812500000002,177.47957404941982,0,2.46,0,0,14.170930147058826,17.769633067498418,17.757794053671798,17.71086757455523,17.612595208274577,17.564290891096753,17.612595208274577,17.71086757455523,17.757794053671798,0,0.82620000000000016,10.199999999999999]
[null,null,null,null,null,19,68400,16.428312500000001,0,0,3.69,1.5,0,12.722430147058823,16.428312500000001,16.428312500000001,16.428312500000001,16.428312500000001,16.428312500000001,16.428312500000001,16.428312500000001,16.428312500000001,0,0.82620000000000016,0]
[null,null,null,null,null,20,72000,15.377812500000003,0,0,4.4279999999999999,1.5,0,11.671930147058827,15.377812500000003,15.377812500000003,15.377812500000003,15.377812500000003,15.377812500000003,15.377812500000003,15.377812500000003,15.377812500000003,0,0.82620000000000016,0]
[null,null,null,null,null,21,75600,14.3548125,0,0,4.92,1.5,0,10.648930147058824,14.3548125,14.3548125,14.3548125,14.3548125,14.3548125,14.3548125,14.3548125,14.3548125,0,0.82620000000000016,0]
[null,null,null,null,null,22,79200,13.320812499999999,0,0,4.0999999999999996,0,0,9.6149301470588213,13.320812499999999,13.320812499999999,13.320812499999999,13.320812499999999,13.320812499999999,13.320812499999999,13.320812499999999,13.320812499999999,0,0.82620000000000016,0]
[null,null,null,null,null,23,82800,12.275812500000002,0,0,4.0999999999999996,0,0,8.5699301470588267,12.275812500000002,12.275812500000002,12.275812500000002,12.275812500000002,12.275812500000002,12.275812500000002,12.275812500000002,12.275812500000002,0,0.82620000000000016,0]
[null,null,null,null,null,24,86400,11.6928125,0,0,4.0999999999999996,0,0,7.9869301470588239,11.6928125,11.6928125,11.6928125,11.6928125,11.6928125,11.6928125,11.6928125,11.6928125,0,0.82620000000000016,0]
[null,null,null,null,null,null,"Valor Variable",{"$f":"+INDIRECT(H132&$C106)+((INDIRECT(H132&$C106+1)-INDIRECT(H132&$C106))/(INDIRECT($C$4&$C106+1)-INDIRECT($C$4&$C106)))*($C$6-INDIRECT($C$4&$C106))","v":11.6928125},{"$f":"+INDIRECT(I132&$C106)+((INDIRECT(I132&$C106+1)-INDIRECT(I132&$C106))/(INDIRECT($C$4&$C106+1)-INDIRECT($C$4&$C106)))*($C$6-INDIRECT($C$4&$C106))","v":0},0,4.0999999999999996,0,{"$f":"+INDIRECT(M132&$C106)+((INDIRECT(M132&$C106+1)-INDIRECT(M132&$C106))/(INDIRECT($C$4&$C106+1)-INDIRECT($C$4&$C106)))*($C$6-INDIRECT($C$4&$C106))","v":0},7.9869301470588239,11.6928125,11.6928125,11.6928125,11.6928125,11.6928125,11.6928125,11.6928125,11.6928125,{"$f":"+INDIRECT(W132&$C106)","v":0},0.82620000000000016,0]
[null,null,null,null,null,null,null,{"$f":"MID(ADDRESS(ROW(),COLUMN()),2,1)","v":"H"},{"$f":"MID(ADDRESS(ROW(),COLUMN()),2,1)","v":"I"},"J","K","L","M","N","O","P","Q","R","S","T","U","V","W","X","Y"]
[]
[]
[]
[null,null,null,null,null,null,null,null,"Rad Ventanas: Sol Incidente*FS*FAV*FAR [W]"]
[null,null,null,null,"Mes","Tiempo [hrs]","Tiempo [s]","T° exterior","Difuso","Directo","Qgen Pers [W/m2]","Qgen Ilum [W/m2]","Qgen Equip [W/m2]","TsolH","TsolN","TsolNE","TsolE","TsolSE","TsolS","TsolSO","TsolO","TsolNO","Clima [0, 1 o 2]","N [RAH]","G total [W/m2]"]
[null,"Fila inicial intervalo",{"$f":"TRUNC($C$6/3600,0)+10+32*(E139-1)","v":138},null,"Mayo",0,0,9.597306451612905,0,0,4.0999999999999996,0,0,5.8914240986717283,9.597306451612905,9.597306451612905,9.597306451612905,9.597306451612905,9.597306451612905,9.597306451612905,9.597306451612905,9.597306451612905,0,0.82620000000000016,0]
[null,null,null,null,5,1,3600,8.7312741935483889,0,0,4.0999999999999996,0,0,5.0253918406072122,8.7312741935483889,8.7312741935483889,8.7312741935483889,8.7312741935483889,8.7312741935483889,8.7312741935483889,8.7312741935483889,8.7312741935483889,0,0.82620000000000016,0]
[null,null,null,null,"Tmax Dia",2,7200,7.8703064516129029,0,0,4.0999999999999996,0,0,4.1644240986717262,7.8703064516129029,7.8703064516129029,7.8703064516129029,7.8703064516129029,7.8703064516129029,7.8703064516129029,7.8703064516129029,7.8703064516129029,0,0.82620000000000016,0]
[null,null,null,null,24.728298387096771,3,10800,7.389177419354839,0,0,4.0999999999999996,0,0,3.6832950664136623,7.389177419354839,7.389177419354839,7.389177419354839,7.389177419354839,7.389177419354839,7.389177419354839,7.389177419354839,7.389177419354839,0,0.82620000000000016,0]
[null,null,null,null,"Tmin Dia",4,14400,6.9485645161290321,0,0,4.0999999999999996,0,0,3.2426821631878555,6.9485645161290321,6.9485645161290321,6.9485645161290321,6.9485645161290321,6.9485645161290321,6.9485645161290321,6.9485645161290321,6.9485645161290321,0,0.82620000000000016,0]
[null,null,null,null,19.728298387096771,5,18000,6.6295000000000011,0,0,4.0999999999999996,0,0,2.9236176470588244,6.6295000000000011,6.6295000000000011,6.6295000000000011,6.6295000000000011,6.6295000000000011,6.6295000000000011,6.6295000000000011,6.6295000000000011,0,0.82620000000000016,0]
[null,null,null,null,"Tmax Noche",6,21600,6.6649516129032254,0,0,3.28,0,0,2.9590692599620487,6.6649516129032254,6.6649516129032254,6.6649516129032254,6.6649516129032254,6.6649516129032254,6.6649516129032254,6.6649516129032254,6.6649516129032254,0,0.82620000000000016,0]
[null,null,null,null,24.728298387096771,7,25200,8.5084354838709686,16.277380289162476,0,3.9359999999999999,1.5,0,4.8410730550284642,8.5476829381984594,8.5418615483699281,8.5323554076811661,8.5206844802573674,8.5177340412623774,8.5206844802573674,8.5323554076811661,8.5418615483699281,0,0.82620000000000016,0.93548387096774188]
[null,null,null,null,"Tmin Noche",8,28800,11.091338709677421,982.81699608012059,192.42163773751994,1.968,0,0,11.171035104364329,14.948416117723976,14.376314013885503,13.442089842748597,12.295119389030365,12.005162453315855,12.295119389030365,13.442089842748597,14.376314013885501,0,0.82620000000000016,91.935483870967744]
[null,null,null,null,17.728298387096771,9,32400,13.755274193548386,1969.5630149886592,676.71485883122352,1.23,0,0,19.844078747628082,23.734954476683576,22.254715559594139,19.837533441010436,16.869898309179476,16.119672890246562,16.869898309179476,19.837533441010436,22.254715559594139,0,0.82620000000000016,237.87096774193549]
[null,null,null,null,"Tsuelo",10,36000,16.079887096774193,2912.5284938091063,1103.2290622239427,1.23,0,0,27.63586432637571,31.629999173425034,29.32352437584467,25.557125875366403,20.933023940902377,19.764039663232296,20.933023940902377,25.557125875366403,29.323524375844666,0,0.82620000000000016,370.64516129032256]
[null,null,null,null,13.052150537634409,11,39600,17.928435483870974,3509.1786747532346,1423.2898027009094,1.23,0,0,33.324450664136634,37.391112748824483,34.504305606613578,29.790243218852225,24.002670553967356,22.539558030279501,24.002670553967356,29.790243218852225,34.50430560661357,0,0.82620000000000016,463.90322580645159]
[null,null,null,null,"Infil RAH",12,43200,19.321177419354836,3866.7197521393205,1181.4896660930656,1.23,0,0,36.526300759013282,40.627131677206378,37.466919950634775,32.306396748456422,25.970692940426201,24.369011523249519,25.970692940426201,32.306396748456422,37.466919950634775,0,0.82620000000000016,507.83870967741933]
[null,null,null,null,0,13,46800,20.192274193548386,4069.9063612661075,1927.3377747859165,1.23,0,0,38.037625237191648,42.150548209532715,38.893580969259304,33.575059152874637,27.045376482145407,25.394656734086478,27.045376482145407,33.575059152874637,38.893580969259304,0,3.8262,523.38709677419354]
[null,null,null,null,"Cat Mes",14,50400,20.399919354838715,3515.3528534836064,1901.5654845057397,1.23,0,0,36.773543643263764,40.858669943414071,37.824119942106634,32.86879825962361,26.785025505638171,25.24703287504299,26.785025505638171,32.86879825962361,37.824119942106634,0,3.8262,487.64516129032256]
[null,null,null,null,"v",15,54000,19.761790322580637,2874.3608434758976,1475.8931567114801,1.23,0,0,31.985888994307391,35.992642727739351,33.585196927270999,29.653916055535937,24.827383897134972,23.60722476379317,24.827383897134972,29.653916055535937,33.585196927270992,0,3.8262,386.87096774193549]
[null,null,null,null,null,16,57600,18.262693548387102,2007.7306653218682,926.51383557236966,1.476,0,0,25.038215370018978,28.942061206946875,27.358040960845337,24.771387299637855,21.595687703044675,20.792863078580389,21.595687703044675,24.771387299637855,27.358040960845337,0,0.82620000000000016,254.54838709677421]
[null,null,null,null,null,17,61200,16.449596774193548,1018.7394905113756,288.22011296664817,2.46,0,0,16.93707305502846,20.72215585391389,20.088427312925099,19.053569169669231,17.783047863568019,17.461856970216893,17.783047863568019,19.053569169669231,20.088427312925095,0,0.82620000000000016,101.83870967741936]
[null,null,null,null,null,18,64800,15.456951612903229,30.309604676371507,0,2.46,0,0,11.82279601518027,15.530033079582006,15.519193250246119,15.501492160687736,15.479760088933073,15.474266168045851,15.479760088933073,15.501492160687736,15.519193250246119,0,0.82620000000000016,1.7419354838709677]
[null,null,null,null,null,19,68400,14.433919354838709,0,0,3.69,1.5,0,10.728037001897533,14.433919354838709,14.433919354838709,14.433919354838709,14.433919354838709,14.433919354838709,14.433919354838709,14.433919354838709,14.433919354838709,0,0.82620000000000016,0]
[null,null,null,null,null,20,72000,13.441274193548386,0,0,4.4279999999999999,1.5,0,9.7353918406072104,13.441274193548386,13.441274193548386,13.441274193548386,13.441274193548386,13.441274193548386,13.441274193548386,13.441274193548386,13.441274193548386,0,0.82620000000000016,0]
[null,null,null,null,null,21,75600,12.448629032258065,0,0,4.92,1.5,0,8.7427466793168875,12.448629032258065,12.448629032258065,12.448629032258065,12.448629032258065,12.448629032258065,12.448629032258065,12.448629032258065,12.448629032258065,0,0.82620000000000016,0]
[null,null,null,null,null,22,79200,11.445854838709678,0,0,4.0999999999999996,0,0,7.7399724857685017,11.445854838709678,11.445854838709678,11.445854838709678,11.445854838709678,11.445854838709678,11.445854838709678,11.445854838709678,11.445854838709678,0,0.82620000000000016,0]
[null,null,null,null,null,23,82800,10.443080645161293,0,0,4.0999999999999996,0,0,6.7371982922201168,10.443080645161293,10.443080645161293,10.443080645161293,10.443080645161293,10.443080645161293,10.443080645161293,10.443080645161293,10.443080645161293,0,0.82620000000000016,0]
[null,null,null,null,null,24,86400,9.597306451612905,0,0,4.0999999999999996,0,0,5.8914240986717283,9.597306451612905,9.597306451612905,9.597306451612905,9.597306451612905,9.597306451612905,9.597306451612905,9.597306451612905,9.597306451612905,0,0.82620000000000016,0]
[null,null,null,null,null,null,"Valor Variable",{"$f":"+INDIRECT(H164&$C138)+((INDIRECT(H164&$C138+1)-INDIRECT(H164&$C138))/(INDIRECT($C$4&$C138+1)-INDIRECT($C$4&$C138)))*($C$6-INDIRECT($C$4&$C138))","v":9.597306451612905},{"$f":"+INDIRECT(I164&$C138)+((INDIRECT(I164&$C138+1)-INDIRECT(I164&$C138))/(INDIRECT($C$4&$C138+1)-INDIRECT($C$4&$C138)))*($C$6-INDIRECT($C$4&$C138))","v":0},0,4.0999999999999996,0,{"$f":"+INDIRECT(M164&$C138)+((INDIRECT(M164&$C138+1)-INDIRECT(M164&$C138))/(INDIRECT($C$4&$C138+1)-INDIRECT($C$4&$C138)))*($C$6-INDIRECT($C$4&$C138))","v":0},5.8914240986717283,9.597306451612905,9.597306451612905,9.597306451612905,9.597306451612905,9.597306451612905,9.597306451612905,9.597306451612905,9.597306451612905,{"$f":"+INDIRECT(W164&$C138)","v":0},0.82620000000000016,0]
[null,null,null,null,null,null,null,{"$f":"MID(ADDRESS(ROW(),COLUMN()),2,1)","v":"H"},{"$f":"MID(ADDRESS(ROW(),COLUMN()),2,1)","v":"I"},"J","K","L","M","N","O","P","Q","R","S","T","U","V","W","X","Y"]
[]
[]
[]
[null,null,null,null,null,null,null,null,"Rad Ventanas: Sol Incidente*FS*FAV*FAR [W]"]
[null,null,null,null,"Mes","Tiempo [hrs]","Tiempo [s]","T° exterior","Difuso","Directo","Qgen Pers [W/m2]","Qgen Ilum [W/m2]","Qgen Equip [W/m2]","TsolH","TsolN","TsolNE","TsolE","TsolSE","TsolS","TsolSO","TsolO","TsolNO","Clima [0, 1 o 2]","N [RAH]","G total [W/m2]"]
[null,"Fila inicial intervalo",{"$f":"TRUNC($C$6/3600,0)+10+32*(E171-1)","v":170},null,"Junio",0,0,8.1411833333333341,0,0,4.0999999999999996,0,0,4.4353009803921575,8.1411833333333341,8.1411833333333341,8.1411833333333341,8.1411833333333341,8.1411833333333341,8.1411833333333341,8.1411833333333341,8.1411833333333341,0,0.82620000000000016,0]
[null,null,null,null,6,1,3600,7.2262499999999994,0,0,4.0999999999999996,0,0,3.5203676470588228,7.2262499999999994,7.2262499999999994,7.2262499999999994,7.2262499999999994,7.2262499999999994,7.2262499999999994,7.2262499999999994,7.2262499999999994,0,0.82620000000000016,0]
[null,null,null,null,"Tmax Dia",2,7200,6.3161833333333313,0,0,4.0999999999999996,0,0,2.6103009803921546,6.3161833333333313,6.3161833333333313,6.3161833333333313,6.3161833333333313,6.3161833333333313,6.3161833333333313,6.3161833333333313,6.3161833333333313,0,0.82620000000000016,0]
[null,null,null,null,24.289787499999999,3,10800,5.8733166666666659,0,0,4.0999999999999996,0,0,2.1674343137254892,5.8733166666666659,5.8733166666666659,5.8733166666666659,5.8733166666666659,5.8733166666666659,5.8733166666666659,5.8733166666666659,5.8733166666666659,0,0.82620000000000016,0]
[null,null,null,null,"Tmin Dia",4,14400,5.3963833333333326,0,0,4.0999999999999996,0,0,1.690500980392156,5.3963833333333326,5.3963833333333326,5.3963833333333326,5.3963833333333326,5.3963833333333326,5.3963833333333326,5.3963833333333326,5.3963833333333326,0,0.82620000000000016,0]
[null,null,null,null,19.289787499999999,5,18000,5.0995166666666654,0,0,4.0999999999999996,0,0,1.3936343137254887,5.0995166666666654,5.0995166666666654,5.0995166666666654,5.0995166666666654,5.0995166666666654,5.0995166666666654,5.0995166666666654,5.0995166666666654,0,0.82620000000000016,0]
[null,null,null,null,"Tmax Noche",6,21600,5.0849166666666674,0,0,3.28,0,0,1.3790343137254908,5.0849166666666674,5.0849166666666674,5.0849166666666674,5.0849166666666674,5.0849166666666674,5.0849166666666674,5.0849166666666674,5.0849166666666674,0,0.82620000000000016,0]
[null,null,null,null,24.289787499999999,7,25200,6.58385,0.57999860800463998,0,3.9359999999999999,1.5,0,2.8793401960784308,6.5854987051202674,6.5851885700291959,6.5847187517874781,6.5842338886082619,6.584148581707038,6.5842338886082619,6.5847187517874781,6.5851885700291959,0,0.82620000000000016,3.3333333333333333E-2]
[null,null,null,null,"Tmin Noche",8,28800,9.0171833333333318,677.43837414941936,169.95085290479108,1.968,0,0,8.0783598039215683,12.340972855791964,11.715740512191564,10.768586936889307,9.7911027675901643,9.6191240547214978,9.7911027675901643,10.768586936889307,11.715740512191564,0,0.82620000000000016,67.2]
[null,null,null,null,17.289787499999999,9,32400,11.523516666666668,1481.3164448438504,675.99555052813696,1.23,0,0,15.952732352941176,21.295391914490235,19.457221229708701,16.672608511049734,13.798824447837424,13.293210444279596,13.798824447837424,16.672608511049734,19.457221229708701,0,0.82620000000000016,197.56666666666666]
[null,null,null,null,"Tsuelo",10,36000,13.874116666666668,2116.9949192169356,1155.7860479975586,1.23,0,0,23.093528431372548,29.39997278422269,26.479430631601176,22.055152249348517,17.489195690672911,16.685860601841451,17.489195690672911,22.055152249348517,26.479430631601176,0,0.82620000000000016,313.89999999999998]
[null,null,null,null,11.332499999999998,11,39600,16.025183333333334,2630.2936873010422,1541.181673157834,1.23,0,0,29.098712745098037,36.180603428599596,32.389201940248952,26.645673935253864,20.718221569340166,19.675344701870209,20.718221569340166,26.645673935253864,32.389201940248952,0,0.82620000000000016,407.5]
[null,null,null,null,"Infil RAH",12,43200,17.601983333333333,2988.7328270479097,1535.2385959621986,1.23,0,0,33.931199019607845,41.668131973873344,37.141090049500804,30.283153175152066,23.205605348138384,21.960380510963823,23.205605348138384,30.283153175152066,37.141090049500804,0,0.82620000000000016,486.56666666666666]
[null,null,null,null,0,13,46800,18.395250000000001,3241.0322215299284,2299.7698914756934,1.23,0,0,35.075838235294121,42.883467151328404,38.277030643641524,31.298820299413141,24.097147498520204,22.830084094632163,24.097147498520204,31.298820299413141,38.277030643641524,0,0.82620000000000016,495.1]
[null,null,null,null,"Cat Mes",14,50400,18.589916666666667,3051.3726767124108,1870.8435695685157,1.23,0,0,32.449916666666667,39.690044795846021,35.720935900311332,29.708202042812182,23.502923075207807,22.411165353336191,23.502923075207807,29.708202042812182,35.720935900311332,0,0.82620000000000016,426.6]
[null,null,null,null,"i",15,54000,17.957250000000002,2196.4547285135714,1651.4159835928531,1.23,0,0,28.580779411764706,35.169731455589343,31.93192110480156,27.027018661272013,21.965047070258599,21.074443021474437,21.965047070258599,27.027018661272013,31.93192110480156,0,0.82620000000000016,348]
[null,null,null,null,null,16,57600,16.424249999999997,1538.1563084283052,1022.9197757983088,1.476,0,0,22.014642156862742,27.590929779569599,25.490384807741471,22.308305856589588,19.024327543760673,18.446543901766887,19.024327543760673,22.308305856589588,25.490384807741471,0,0.82620000000000016,225.76666666666668]
[null,null,null,null,null,17,61200,14.667383333333335,720.35827114176277,277.5113587339261,2.46,0,0,14.200716666666668,18.558327417163877,17.826408602234835,16.717637551781799,15.573360448832405,15.372036161942498,15.573360448832405,16.717637551781799,17.826408602234835,0,0.82620000000000016,78.666666666666671]
[null,null,null,null,null,18,64800,13.718383333333332,6.9599832960556798,0,2.46,1.5,0,10.028971568627448,13.738167794776539,13.734446173683679,13.728808354783069,13.72298999663248,13.721966313817784,13.72298999663248,13.728808354783069,13.734446173683679,0,0.82620000000000016,0.4]
[null,null,null,null,null,19,68400,12.774249999999999,0,0,3.69,1.5,0,9.068367647058821,12.774249999999999,12.774249999999999,12.774249999999999,12.774249999999999,12.774249999999999,12.774249999999999,12.774249999999999,12.774249999999999,0,0.82620000000000016,0]
[null,null,null,null,null,20,72000,11.83498333333333,0,0,4.4279999999999999,1.5,0,8.1291009803921526,11.83498333333333,11.83498333333333,11.83498333333333,11.83498333333333,11.83498333333333,11.83498333333333,11.83498333333333,11.83498333333333,0,0.82620000000000016,0]
[null,null,null,null,null,21,75600,10.905449999999997,0,0,4.92,1.5,0,7.1995676470588199,10.905449999999997,10.905449999999997,10.905449999999997,10.905449999999997,10.905449999999997,10.905449999999997,10.905449999999997,10.905449999999997,0,0.82620000000000016,0]
[null,null,null,null,null,22,79200,9.9467166666666653,0,0,4.0999999999999996,0,0,6.2408343137254887,9.9467166666666653,9.9467166666666653,9.9467166666666653,9.9467166666666653,9.9467166666666653,9.9467166666666653,9.9467166666666653,9.9467166666666653,0,0.82620000000000016,0]
[null,null,null,null,null,23,82800,9.0025833333333303,0,0,4.0999999999999996,0,0,5.2967009803921536,9.0025833333333303,9.0025833333333303,9.0025833333333303,9.0025833333333303,9.0025833333333303,9.0025833333333303,9.0025833333333303,9.0025833333333303,0,0.82620000000000016,0]
[null,null,null,null,null,24,86400,8.1411833333333341,0,0,4.0999999999999996,0,0,4.4353009803921575,8.1411833333333341,8.1411833333333341,8.1411833333333341,8.1411833333333341,8.1411833333333341,8.1411833333333341,8.1411833333333341,8.1411833333333341,0,0.82620000000000016,0]
[null,null,null,null,null,null,"Valor Variable",{"$f":"+INDIRECT(H196&$C170)+((INDIRECT(H196&$C170+1)-INDIRECT(H196&$C170))/(INDIRECT($C$4&$C170+1)-INDIRECT($C$4&$C170)))*($C$6-INDIRECT($C$4&$C170))","v":8.1411833333333341},{"$f":"+INDIRECT(I196&$C170)+((INDIRECT(I196&$C170+1)-INDIRECT(I196&$C170))/(INDIRECT($C$4&$C170+1)-INDIRECT($C$4&$C170)))*($C$6-INDIRECT($C$4&$C170))","v":0},0,4.0999999999999996,0,{"$f":"+INDIRECT(M196&$C170)+((INDIRECT(M196&$C170+1)-INDIRECT(M196&$C170))/(INDIRECT($C$4&$C170+1)-INDIRECT($C$4&$C170)))*($C$6-INDIRECT($C$4&$C170))","v":0},4.4353009803921575,8.1411833333333341,8.1411833333333341,8.1411833333333341,8.1411833333333341,8.1411833333333341,8.1411833333333341,8.1411833333333341,8.1411833333333341,{"$f":"+INDIRECT(W196&$C170)","v":0},0.82620000000000016,0]
[null,null,null,null,null,null,null,{"$f":"MID(ADDRESS(ROW(),COLUMN()),2,1)","v":"H"},{"$f":"MID(ADDRESS(ROW(),COLUMN()),2,1)","v":"I"},"J","K","L","M","N","O","P","Q","R","S","T","U","V","W","X","Y"]
[]
[]
[]
[null,null,null,null,null,null,null,null,"Rad Ventanas: Sol Incidente*FS*FAV*FAR [W]"]
[null,null,null,null,"Mes","Tiempo [hrs]","Tiempo [s]","T° exterior","Difuso","Directo","Qgen Pers [W/m2]","Qgen Ilum [W/m2]","Qgen Equip [W/m2]","TsolH","TsolN","TsolNE","TsolE","TsolSE","TsolS","TsolSO","TsolO","TsolNO","Clima [0, 1 o 2]","N [RAH]","G total [W/m2]"]
[null,"Fila inicial intervalo",{"$f":"TRUNC($C$6/3600,0)+10+32*(E203-1)","v":202},null,"Julio",0,0,7.3976303763440843,0,0,4.0999999999999996,0,0,3.6917480234029076,7.3976303763440843,7.3976303763440843,7.3976303763440843,7.3976303763440843,7.3976303763440843,7.3976303763440843,7.3976303763440843,7.3976303763440843,0,0.82620000000000016,0]
[null,null,null,null,7,1,3600,6.487243279569892,0,0,4.0999999999999996,0,0,2.7813609266287154,6.487243279569892,6.487243279569892,6.487243279569892,6.487243279569892,6.487243279569892,6.487243279569892,6.487243279569892,6.487243279569892,0,0.82620000000000016,0]
[null,null,null,null,"Tmax Dia",2,7200,5.5856948924731187,0,0,4.0999999999999996,0,0,1.8798125395319421,5.5856948924731187,5.5856948924731187,5.5856948924731187,5.5856948924731187,5.5856948924731187,5.5856948924731187,5.5856948924731187,5.5856948924731187,0,0.82620000000000016,0]
[null,null,null,null,24.15972379032258,3,10800,5.1216626344086018,0,0,4.0999999999999996,0,0,1.4157802814674252,5.1216626344086018,5.1216626344086018,5.1216626344086018,5.1216626344086018,5.1216626344086018,5.1216626344086018,5.1216626344086018,5.1216626344086018,0,0.82620000000000016,0]
[null,null,null,null,"Tmin Dia",4,14400,4.6885658602150526,0,0,4.0999999999999996,0,0,0.98268350727387599,4.6885658602150526,4.6885658602150526,4.6885658602150526,4.6885658602150526,4.6885658602150526,4.6885658602150526,4.6885658602150526,4.6885658602150526,0,0.82620000000000016,0]
[null,null,null,null,19.15972379032258,5,18000,4.3571142473118289,0,0,4.0999999999999996,0,0,0.65123189437065232,4.3571142473118289,4.3571142473118289,4.3571142473118289,4.3571142473118289,4.3571142473118289,4.3571142473118289,4.3571142473118289,4.3571142473118289,0,0.82620000000000016,0]
[null,null,null,null,"Tmax Noche",6,21600,4.3526948924731199,0,0,3.28,0,0,0.64681253953194329,4.3526948924731199,4.3526948924731199,4.3526948924731199,4.3526948924731199,4.3526948924731199,4.3526948924731199,4.3526948924731199,4.3526948924731199,0,0.82620000000000016,0]
[null,null,null,null,24.15972379032258,7,25200,6.0143723118279571,6.7354677058603345,0,3.9359999999999999,1.5,0,2.3244292378241616,6.0319724292164913,6.028988099316182,6.0243504421888829,6.0192138600966985,6.0181495675504193,6.0192138600966985,6.0243504421888829,6.028988099316182,0,0.82620000000000016,0.38709677419354838]
[null,null,null,null,"Tmin Noche",8,28800,8.524565860215052,710.59184296826527,228.09746376830844,1.968,0,0,8.1433514389626787,12.195657012173454,11.573175533800537,10.605837551331561,9.5344321366033515,9.312438449658595,9.5344321366033515,10.605837551331561,11.573175533800535,0,0.82620000000000016,80.741935483870961]
[null,null,null,null,17.15972379032258,9,32400,11.246888440860214,1425.112708764949,793.45463750608837,1.23,0,0,16.629051628716002,21.281888705222734,19.580323273729526,16.936085768314928,14.007377878754239,13.400553745283997,14.007377878754239,16.936085768314928,19.580323273729526,0,0.82620000000000016,220.70967741935485]
[null,null,null,null,"Tsuelo",10,36000,13.708469086021507,2026.2532015129839,1394.0313872986353,1.23,0,0,24.839398877292854,30.091245021848657,27.313331272977106,22.996445430316911,18.215143599508245,17.224464621013269,18.215143599508245,22.996445430316911,27.313331272977102,0,0.82620000000000016,360.32258064516128]
[null,null,null,null,10.82244623655914,11,39600,15.723694892473121,2653.7742761089721,1754.5249537230839,1.23,0,0,30.93640836495889,36.613567556214043,33.071416658704869,27.566904120029026,21.470209225113372,20.206982663725377,21.470209225113372,27.566904120029026,33.071416658704862,0,0.82620000000000016,459.45161290322579]
[null,null,null,null,"Infil RAH",12,43200,17.133469086021506,3112.3473690829633,1492.708782673888,1.23,0,0,34.503298308032896,40.405224303010705,36.459194092326292,30.32705195575608,23.535206284364751,22.127945465046956,23.535206284364751,30.32705195575608,36.459194092326285,0,0.82620000000000016,511.83870967741933]
[null,null,null,null,0,13,46800,18.07479166666667,3117.3989698623582,2323.5694124086958,1.23,0,0,35.366252767235935,41.260012973162247,37.328655717821022,31.219315395460022,24.452724586021937,23.050696538390017,24.452724586021937,31.219315395460022,37.328655717821022,0,0.82620000000000016,509.93548387096774]
[null,null,null,null,"Cat Mes",14,50400,18.362049731182797,2913.0897827845947,2234.0619111505102,1.23,0,0,34.645351438962685,40.434063612853592,36.691465223706956,30.875456714647573,24.433754722540172,23.09904317846042,24.433754722540172,30.875456714647573,36.691465223706949,0,0.82620000000000016,485.45161290322579]
[null,null,null,null,"i",15,54000,17.685888440860218,2295.6719097473974,1849.0663551058087,1.23,0,0,30.251353336495892,35.652674941655434,32.606171501756023,27.871896517638973,22.628302298533676,21.541836990873566,22.628302298533676,27.871896517638973,32.606171501756016,0,0.82620000000000016,395.16129032258067]
[null,null,null,null,null,16,57600,16.112598118279571,1567.1188195635045,1114.4250409816627,1.476,0,0,22.647702482605947,27.420673540412725,25.503241579463783,22.52354687517461,19.223292880945888,18.539484919961442,19.223292880945888,22.52354687517461,25.503241579463783,0,0.82620000000000016,248.70967741935485]
[null,null,null,null,null,17,61200,14.274146505376343,782.99812080626396,327.21223244764553,2.46,0,0,14.339231894370648,18.4380409442137,17.731998228632111,16.634805846598784,15.4195761332894,15.167782255048824,15.4195761332894,16.634805846598784,17.731998228632111,0,0.82620000000000016,91.58064516129032]
[null,null,null,null,null,18,64800,13.293049731182794,13.470935411720669,0,2.46,1.5,0,9.6190459361163789,13.328249965959863,13.322281306159244,13.313005991904646,13.302732827720277,13.300604242627719,13.302732827720277,13.313005991904646,13.322281306159244,0,0.82620000000000016,0.77419354838709675]
[null,null,null,null,null,19,68400,12.311952956989243,0,0,3.69,1.5,0,8.6060706040480675,12.311952956989243,12.311952956989243,12.311952956989243,12.311952956989243,12.311952956989243,12.311952956989243,12.311952956989243,12.311952956989243,0,0.82620000000000016,0]
[null,null,null,null,null,20,72000,11.308759408602148,0,0,4.4279999999999999,1.5,0,7.6028770556609713,11.308759408602148,11.308759408602148,11.308759408602148,11.308759408602148,11.308759408602148,11.308759408602148,11.308759408602148,11.308759408602148,0,0.82620000000000016,0]
[null,null,null,null,null,21,75600,10.296727150537633,0,0,4.92,1.5,0,6.5908447975964561,10.296727150537633,10.296727150537633,10.296727150537633,10.296727150537633,10.296727150537633,10.296727150537633,10.296727150537633,10.296727150537633,0,0.82620000000000016,0]
[null,null,null,null,null,22,79200,9.3244690860215016,0,0,4.0999999999999996,0,0,5.618586733080325,9.3244690860215016,9.3244690860215016,9.3244690860215016,9.3244690860215016,9.3244690860215016,9.3244690860215016,9.3244690860215016,9.3244690860215016,0,0.82620000000000016,0]
[null,null,null,null,null,23,82800,8.352211021505374,0,0,4.0999999999999996,0,0,4.6463286685641974,8.352211021505374,8.352211021505374,8.352211021505374,8.352211021505374,8.352211021505374,8.352211021505374,8.352211021505374,8.352211021505374,0,0.82620000000000016,0]
[null,null,null,null,null,24,86400,7.3976303763440843,0,0,4.0999999999999996,0,0,3.6917480234029076,7.3976303763440843,7.3976303763440843,7.3976303763440843,7.3976303763440843,7.3976303763440843,7.3976303763440843,7.3976303763440843,7.3976303763440843,0,0.82620000000000016,0]
[null,null,null,null,null,null,"Valor Variable",{"$f":"+INDIRECT(H228&$C202)+((INDIRECT(H228&$C202+1)-INDIRECT(H228&$C202))/(INDIRECT($C$4&$C202+1)-INDIRECT($C$4&$C202)))*($C$6-INDIRECT($C$4&$C202))","v":7.3976303763440843},{"$f":"+INDIRECT(I228&$C202)+((INDIRECT(I228&$C202+1)-INDIRECT(I228&$C202))/(INDIRECT($C$4&$C202+1)-INDIRECT($C$4&$C202)))*($C$6-INDIRECT($C$4&$C202))","v":0},0,4.0999999999999996,0,{"$f":"+INDIRECT(M228&$C202)+((INDIRECT(M228&$C202+1)-INDIRECT(M228&$C202))/(INDIRECT($C$4&$C202+1)-INDIRECT($C$4&$C202)))*($C$6-INDIRECT($C$4&$C202))","v":0},3.6917480234029076,7.3976303763440843,7.3976303763440843,7.3976303763440843,7.3976303763440843,7.3976303763440843,7.3976303763440843,7.3976303763440843,7.3976303763440843,{"$f":"+INDIRECT(W228&$C202)","v":0},0.82620000000000016,0]
[null,null,null,null,null,null,null,{"$f":"MID(ADDRESS(ROW(),COLUMN()),2,1)","v":"H"},{"$f":"MID(ADDRESS(ROW(),COLUMN()),2,1)","v":"I"},"J","K","L","M","N","O","P","Q","R","S","T","U","V","W","X","Y"]
[]
[]
[]
[null,null,null,null,null,null,null,null,"Rad Ventanas: Sol Incidente*FS*FAV*FAR [W]"]
[null,null,null,null,"Mes","Tiempo [hrs]","Tiempo [s]","T° exterior","Difuso","Directo","Qgen Pers [W/m2]","Qgen Ilum [W/m2]","Qgen Equip [W/m2]","TsolH","TsolN","TsolNE","TsolE","TsolSE","TsolS","TsolSO","TsolO","TsolNO","Clima [0, 1 o 2]","N [RAH]","G total [W/m2]"]
[null,"Fila inicial intervalo",{"$f":"TRUNC($C$6/3600,0)+10+32*(E235-1)","v":234},null,"Agosto",0,0,7.8629704301075254,0,0,4.0999999999999996,0,0,4.1570880771663488,7.8629704301075254,7.8629704301075254,7.8629704301075254,7.8629704301075254,7.8629704301075254,7.8629704301075254,7.8629704301075254,7.8629704301075254,0,0.82620000000000016,0]
[null,null,null,null,8,1,3600,6.9450026881720444,0,0,4.0999999999999996,0,0,3.2391203352308677,6.9450026881720444,6.9450026881720444,6.9450026881720444,6.9450026881720444,6.9450026881720444,6.9450026881720444,6.9450026881720444,6.9450026881720444,0,0.82620000000000016,0]
[null,null,null,null,"Tmax Dia",2,7200,6.0362607526881709,0,0,4.0999999999999996,0,0,2.3303783997469942,6.0362607526881709,6.0362607526881709,6.0362607526881709,6.0362607526881709,6.0362607526881709,6.0362607526881709,6.0362607526881709,6.0362607526881709,0,0.82620000000000016,0]
[null,null,null,null,24.358342741935484,3,10800,5.57035752688172,0,0,4.0999999999999996,0,0,1.8644751739405434,5.57035752688172,5.57035752688172,5.57035752688172,5.57035752688172,5.57035752688172,5.57035752688172,5.57035752688172,5.57035752688172,0,0.82620000000000016,0]
[null,null,null,null,"Tmin Dia",4,14400,5.0952284946236555,0,0,4.0999999999999996,0,0,1.3893461416824788,5.0952284946236555,5.0952284946236555,5.0952284946236555,5.0952284946236555,5.0952284946236555,5.0952284946236555,5.0952284946236555,5.0952284946236555,0,0.82620000000000016,0]
[null,null,null,null,19.358342741935484,5,18000,4.7492607526881718,0,0,4.0999999999999996,0,0,1.0433783997469952,4.7492607526881718,4.7492607526881718,4.7492607526881718,4.7492607526881718,4.7492607526881718,4.7492607526881718,4.7492607526881718,4.7492607526881718,0,0.82620000000000016,0]
[null,null,null,null,"Tmax Noche",6,21600,4.8738091397849468,0,0,3.28,0,0,1.1679267868437702,4.8738091397849468,4.8738091397849468,4.8738091397849468,4.8738091397849468,4.8738091397849468,4.8738091397849468,4.8738091397849468,4.8738091397849468,0,0.82620000000000016,0]
[null,null,null,null,24.358342741935484,7,25200,7.2033252688172045,71.283699887021868,0,3.9359999999999999,0,0,3.6661336179633146,7.3469139639192393,7.3338042185021663,7.3063745821884005,7.2624576023226783,7.2460146116887794,7.2624576023226783,7.3063745821884005,7.3338042185021663,0,0.82620000000000016,4.096774193548387]
[null,null,null,null,"Tmin Noche",8,28800,9.980293010752689,1456.5448913922974,271.65192475691981,1.968,0,0,12.013879348513598,14.865700503161289,14.419659479955222,13.486403901122287,11.992189176714524,11.432739078060363,11.992189176714524,13.486403901122287,14.419659479955222,0,0.82620000000000016,139.38709677419354]
[null,null,null,null,17.358342741935484,9,32400,12.62809946236559,2090.8014336941455,937.40374498969572,1.23,0,0,21.781230392156861,23.573628259867938,22.574294044256295,20.483378224149458,17.135659467613571,15.882237480788547,17.135659467613571,20.483378224149458,22.574294044256295,0,0.82620000000000016,312.29032258064518]
[null,null,null,null,"Tsuelo",10,36000,15.017583333333336,2885.5866229856651,1426.4086871795855,1.23,0,0,30.178494149272613,31.076904791831772,29.610677831956984,26.542878192581146,21.631092507441622,19.792067003788834,21.631092507441622,26.542878192581146,29.610677831956984,0,0.82620000000000016,458.19354838709677]
[null,null,null,null,11.601344086021506,11,39600,16.848905913978491,3485.0432488072347,1817.9903724607075,1.23,0,0,36.733156388361792,36.928710835333902,35.095411003781081,31.259581547619796,25.118120426240047,22.81869118483808,25.118120426240047,31.259581547619796,35.095411003781081,0,0.82620000000000016,572.90322580645159]
[null,null,null,null,"Infil RAH",12,43200,18.177422043010754,3601.2300667333257,1436.2966875802292,1.23,0,0,40.107213314358006,39.998381219934146,38.006112821906591,33.837672027767354,27.163674300141839,24.664857613257944,27.163674300141839,33.837672027767354,38.006112821906591,0,0.82620000000000016,622.58064516129036]
[null,null,null,null,0,13,46800,18.989293010752689,3646.6944737478834,2480.6792631290691,1.23,0,0,41.12098181530677,40.982106373939935,38.974147571948635,34.7728776067882,28.046317824520244,25.527821337822552,28.046317824520244,34.7728776067882,38.974147571948635,0,0.82620000000000016,627.48387096774195]
[null,null,null,null,"Cat Mes",14,50400,19.15074462365591,3298.134019969611,2327.3003291447858,1.23,0,0,39.3936288741303,39.535816849558955,37.674645905702121,33.780501474700543,27.545673545732257,25.211286765187353,27.545673545732257,33.780501474700543,37.674645905702121,0,0.82620000000000016,581.61290322580646]
[null,null,null,null,"i",15,54000,18.477260752688167,2624.0259604080888,1850.3129077279964,1.23,0,0,33.81616018342821,34.688085243813944,33.20802595412902,30.111284808721333,25.153161522778607,23.296786721921546,25.153161522778607,30.111284808721333,33.20802595412902,0,0.82620000000000016,462.51612903225805]
[null,null,null,null,null,16,57600,16.987293010752683,1962.8275472827993,1211.1382739707726,1.476,0,0,26.327710468058182,28.092239178407684,27.078350048592831,24.956980852736066,21.560503874459499,20.288826283859827,21.560503874459499,24.956980852736066,27.078350048592831,0,0.82620000000000016,316.83870967741933]
[null,null,null,null,null,17,61200,15.049873655913979,1446.4416898335069,339.11871671181632,2.46,0,0,17.119323371283997,19.965807878777341,19.516979744340873,18.57789266802391,17.074341262857292,16.511395410288838,17.074341262857292,18.57789266802391,19.516979744340873,0,0.82620000000000016,140.25806451612902]
[null,null,null,null,null,18,64800,14.025809139784947,86.999791200695995,0,2.46,0,0,10.525809139784947,14.201055184988217,14.185055101998877,14.151577986812786,14.09797852319714,14.077910306281751,14.09797852319714,14.151577986812786,14.185055101998877,0,0.82620000000000016,5]
[null,null,null,null,null,19,68400,13.001744623655915,0,0,3.69,1.5,0,9.2958622707147391,13.001744623655915,13.001744623655915,13.001744623655915,13.001744623655915,13.001744623655915,13.001744623655915,13.001744623655915,13.001744623655915,0,0.82620000000000016,0]
[null,null,null,null,null,20,72000,11.977680107526881,0,0,4.4279999999999999,1.5,0,8.2717977545857053,11.977680107526881,11.977680107526881,11.977680107526881,11.977680107526881,11.977680107526881,11.977680107526881,11.977680107526881,11.977680107526881,0,0.82620000000000016,0]
[null,null,null,null,null,21,75600,10.958228494623658,0,0,4.92,1.5,0,7.252346141682481,10.958228494623658,10.958228494623658,10.958228494623658,10.958228494623658,10.958228494623658,10.958228494623658,10.958228494623658,10.958228494623658,0,0.82620000000000016,0]
[null,null,null,null,null,22,79200,9.9249381720430119,0,0,4.0999999999999996,0,0,6.2190558191018352,9.9249381720430119,9.9249381720430119,9.9249381720430119,9.9249381720430119,9.9249381720430119,9.9249381720430119,9.9249381720430119,9.9249381720430119,0,0.82620000000000016,0]
[null,null,null,null,null,23,82800,8.9008736559139781,0,0,4.0999999999999996,0,0,5.1949913029728014,8.9008736559139781,8.9008736559139781,8.9008736559139781,8.9008736559139781,8.9008736559139781,8.9008736559139781,8.9008736559139781,8.9008736559139781,0,0.82620000000000016,0]
[null,null,null,null,null,24,86400,7.8629704301075254,0,0,4.0999999999999996,0,0,4.1570880771663488,7.8629704301075254,7.8629704301075254,7.8629704301075254,7.8629704301075254,7.8629704301075254,7.8629704301075254,7.8629704301075254,7.8629704301075254,0,0.82620000000000016,0]
[null,null,null,null,null,null,"Valor Variable",{"$f":"+INDIRECT(H260&$C234)+((INDIRECT(H260&$C234+1)-INDIRECT(H260&$C234))/(INDIRECT($C$4&$C234+1)-INDIRECT($C$4&$C234)))*($C$6-INDIRECT($C$4&$C234))","v":7.8629704301075254},{"$f":"+INDIRECT(I260&$C234)+((INDIRECT(I260&$C234+1)-INDIRECT(I260&$C234))/(INDIRECT($C$4&$C234+1)-INDIRECT($C$4&$C234)))*($C$6-INDIRECT($C$4&$C234))","v":0},0,4.0999999999999996,0,{"$f":"+INDIRECT(M260&$C234)+((INDIRECT(M260&$C234+1)-INDIRECT(M260&$C234))/(INDIRECT($C$4&$C234+1)-INDIRECT($C$4&$C234)))*($C$6-INDIRECT($C$4&$C234))","v":0},4.1570880771663488,7.8629704301075254,7.8629704301075254,7.8629704301075254,7.8629704301075254,7.8629704301075254,7.8629704301075254,7.8629704301075254,7.8629704301075254,{"$f":"+INDIRECT(W260&$C234)","v":0},0.82620000000000016,0]
[null,null,null,null,null,null,null,{"$f":"MID(ADDRESS(ROW(),COLUMN()),2,1)","v":"H"},{"$f":"MID(ADDRESS(ROW(),COLUMN()),2,1)","v":"I"},"J","K","L","M","N","O","P","Q","R","S","T","U","V","W","X","Y"]
[]
[]
[]
[null,null,null,null,null,null,null,null,"Rad Ventanas: Sol Incidente*FS*FAV*FAR [W]"]
[null,null,null,null,"Mes","Tiempo [hrs]","Tiempo [s]","T° exterior","Difuso","Directo","Qgen Pers [W/m2]","Qgen Ilum [W/m2]","Qgen Equip [W/m2]","TsolH","TsolN","TsolNE","TsolE","TsolSE","TsolS","TsolSO","TsolO","TsolNO","Clima [0, 1 o 2]","N [RAH]","G total [W/m2]"]
[null,"Fila inicial intervalo",{"$f":"TRUNC($C$6/3600,0)+10+32*(E267-1)","v":266},null,"Septiembre",0,0,9.0823722222222223,0,0,4.0999999999999996,0,0,5.3764898692810457,9.0823722222222223,9.0823722222222223,9.0823722222222223,9.0823722222222223,9.0823722222222223,9.0823722222222223,9.0823722222222223,9.0823722222222223,0,0.82620000000000016,0]
[null,null,null,null,9,1,3600,8.1349055555555552,0,0,4.0999999999999996,0,0,4.4290232026143785,8.1349055555555552,8.1349055555555552,8.1349055555555552,8.1349055555555552,8.1349055555555552,8.1349055555555552,8.1349055555555552,8.1349055555555552,0,0.82620000000000016,0]
[null,null,null,null,"Tmax Dia",2,7200,7.2938388888888896,0,0,4.0999999999999996,0,0,3.587956535947713,7.2938388888888896,7.2938388888888896,7.2938388888888896,7.2938388888888896,7.2938388888888896,7.2938388888888896,7.2938388888888896,7.2938388888888896,0,0.82620000000000016,0]
[null,null,null,null,24.745352083333334,3,10800,6.7871722222222219,0,0,4.0999999999999996,0,0,3.0812898692810453,6.7871722222222219,6.7871722222222219,6.7871722222222219,6.7871722222222219,6.7871722222222219,6.7871722222222219,6.7871722222222219,6.7871722222222219,0,0.82620000000000016,0]
[null,null,null,null,"Tmin Dia",4,14400,6.3210388888888893,0,0,4.0999999999999996,0,0,2.6151565359477127,6.3210388888888893,6.3210388888888893,6.3210388888888893,6.3210388888888893,6.3210388888888893,6.3210388888888893,6.3210388888888893,6.3210388888888893,0,0.82620000000000016,0]
[null,null,null,null,19.745352083333334,5,18000,6.0626388888888867,0,0,4.0999999999999996,0,0,2.3567565359477101,6.0626388888888867,6.0626388888888867,6.0626388888888867,6.0626388888888867,6.0626388888888867,6.0626388888888867,6.0626388888888867,6.0626388888888867,0,0.82620000000000016,0]
[null,null,null,null,"Tmax Noche",6,21600,6.7466388888888895,0,0,3.28,0,0,3.0407565359477129,6.7466388888888895,6.7466388888888895,6.7466388888888895,6.7466388888888895,6.7466388888888895,6.7466388888888895,6.7466388888888895,6.7466388888888895,0,0.82620000000000016,0]
[null,null,null,null,24.745352083333334,7,25200,9.3914388888888904,408.31902003526653,0,3.9359999999999999,0,0,6.9853604575163404,10.140617489360737,10.212689238705156,10.166054815330918,9.9172962168881149,9.7228686716767072,9.9172962168881149,10.166054815330918,10.212689238705156,0,0.82620000000000016,31.566666666666666]
[null,null,null,null,"Tmin Noche",8,28800,11.990638888888888,1905.8754259032467,271.65192475691981,1.968,0,0,17.388874183006532,17.238053521338479,17.742860188077152,17.416222246956437,15.673861335160126,14.312047283008839,15.673861335160126,17.416222246956437,17.742860188077152,0,0.82620000000000016,221.1]
[null,null,null,null,17.745352083333334,9,32400,14.488505555555554,2146.5748482251724,937.40374498969572,1.23,0,0,27.111838888888887,23.900308945010213,24.805734079065697,24.219873746559564,21.094761765911187,18.652201570156045,21.094761765911187,24.219873746559564,24.805734079065697,0,0.82620000000000016,396.56666666666666]
[null,null,null,null,"Tsuelo",10,36000,16.601305555555555,3054.272669752434,1426.4086871795855,1.23,0,0,35.924050653594776,29.874503611222551,31.151398870462941,30.325176742297195,25.917920391005399,22.473247367185969,25.917920391005399,30.325176742297195,31.151398870462941,0,0.82620000000000016,559.26666666666665]
[null,null,null,null,13.119027777777779,11,39600,18.29357222222222,3716.6310800937326,1817.9903724607075,1.23,0,0,41.891807516339867,34.031069475850998,35.545032844075401,34.565414486964826,29.339907835620942,25.255697532674233,29.339907835620942,34.565414486964826,35.545032844075401,0,0.82620000000000016,663.1]
[null,null,null,null,"Infil RAH",12,43200,19.545038888888893,4174.2499818093938,1436.2966875802292,1.23,0,0,45.655038888888896,36.730262477114792,38.383498602784066,37.313763038941858,31.607550753859506,27.147625131232886,31.607550753859506,37.313763038941858,38.383498602784066,0,0.82620000000000016,724.1]
[null,null,null,null,0,13,46800,20.330372222222227,4111.6101321448923,2480.6792631290691,1.23,0,0,46.734097712418304,37.684892769794459,39.354415436498265,38.274141576349734,32.511715626994146,28.007853895945935,32.511715626994146,38.274141576349734,39.354415436498265,0,3.8262,731.23333333333335]
[null,null,null,null,"Cat Mes",14,50400,20.614105555555554,3861.6307320948927,2327.3003291447858,1.23,0,0,45.503909477124182,37.096034765936182,38.681613251513383,37.655655937280159,32.18296677153851,27.90556077688754,32.18296677153851,37.655655937280159,38.681613251513383,0,3.8262,694.4666666666667]
[null,null,null,null,"v",15,54000,20.188505555555558,3021.2127490961693,1850.3129077279964,1.23,0,0,40.896152614379091,34.259930863467638,35.613616402632545,34.737706699826248,30.065405548292855,26.41357582635483,30.065405548292855,34.737706699826248,35.613616402632545,0,3.8262,592.9]
[null,null,null,null,null,16,57600,18.967438888888896,2129.1748899850331,1211.1382739707726,1.476,0,0,33.259791830065367,29.341228738928315,30.339197956619294,29.693456463793126,26.248924783349132,23.556708943478814,26.248924783349132,29.693456463793126,30.339197956619294,0,0.82620000000000016,437.1]
[null,null,null,null,null,17,61200,17.097838888888891,1868.175516382945,339.11871671181632,2.46,0,0,23.235878104575164,22.771660348850965,23.31748778950373,22.964307130116154,21.080361334940047,19.607885776063366,21.080361334940047,22.964307130116154,23.31748778950373,0,0.82620000000000016,239.06666666666666]
[null,null,null,null,null,18,64800,15.836238888888889,441.95893929953559,0,2.46,0,0,13.601729084967321,16.684305900193873,16.765890816030428,16.71310084574829,16.431507163033736,16.211416003090093,16.431507163033736,16.71310084574829,16.765890816030428,0,0.82620000000000016,35.733333333333334]
[null,null,null,null,null,19,68400,14.620238888888888,0,0,3.69,1.5,0,10.914356535947711,14.620238888888888,14.620238888888888,14.620238888888888,14.620238888888888,14.620238888888888,14.620238888888888,14.620238888888888,14.620238888888888,0,0.82620000000000016,0]
[null,null,null,null,null,20,72000,13.424505555555553,0,0,4.4279999999999999,1.5,0,9.7186232026143777,13.424505555555553,13.424505555555553,13.424505555555553,13.424505555555553,13.424505555555553,13.424505555555553,13.424505555555553,13.424505555555553,0,0.82620000000000016,0]
[null,null,null,null,null,21,75600,12.208505555555551,0,0,4.92,1.5,0,8.5026232026143731,12.208505555555551,12.208505555555551,12.208505555555551,12.208505555555551,12.208505555555551,12.208505555555551,12.208505555555551,12.208505555555551,0,0.82620000000000016,0]
[null,null,null,null,null,22,79200,10.997572222222221,0,0,4.0999999999999996,0,0,7.2916898692810443,10.997572222222221,10.997572222222221,10.997572222222221,10.997572222222221,10.997572222222221,10.997572222222221,10.997572222222221,10.997572222222221,0,0.82620000000000016,0]
[null,null,null,null,null,23,82800,9.8322388888888899,0,0,4.0999999999999996,0,0,6.1263565359477132,9.8322388888888899,9.8322388888888899,9.8322388888888899,9.8322388888888899,9.8322388888888899,9.8322388888888899,9.8322388888888899,9.8322388888888899,0,0.82620000000000016,0]
[null,null,null,null,null,24,86400,9.0823722222222223,0,0,4.0999999999999996,0,0,5.3764898692810457,9.0823722222222223,9.0823722222222223,9.0823722222222223,9.0823722222222223,9.0823722222222223,9.0823722222222223,9.0823722222222223,9.0823722222222223,0,0.82620000000000016,0]
[null,null,null,null,null,null,"Valor Variable",{"$f":"+INDIRECT(H292&$C266)+((INDIRECT(H292&$C266+1)-INDIRECT(H292&$C266))/(INDIRECT($C$4&$C266+1)-INDIRECT($C$4&$C266)))*($C$6-INDIRECT($C$4&$C266))","v":9.0823722222222223},{"$f":"+INDIRECT(I292&$C266)+((INDIRECT(I292&$C266+1)-INDIRECT(I292&$C266))/(INDIRECT($C$4&$C266+1)-INDIRECT($C$4&$C266)))*($C$6-INDIRECT($C$4&$C266))","v":0},0,4.0999999999999996,0,{"$f":"+INDIRECT(M292&$C266)+((INDIRECT(M292&$C266+1)-INDIRECT(M292&$C266))/(INDIRECT($C$4&$C266+1)-INDIRECT($C$4&$C266)))*($C$6-INDIRECT($C$4&$C266))","v":0},5.3764898692810457,9.0823722222222223,9.0823722222222223,9.0823722222222223,9.0823722222222223,9.0823722222222223,9.0823722222222223,9.0823722222222223,9.0823722222222223,{"$f":"+INDIRECT(W292&$C266)","v":0},0.82620000000000016,0]
[null,null,null,null,null,null,null,{"$f":"MID(ADDRESS(ROW(),COLUMN()),2,1)","v":"H"},{"$f":"MID(ADDRESS(ROW(),COLUMN()),2,1)","v":"I"},"J","K","L","M","N","O","P","Q","R","S","T","U","V","W","X","Y"]
[]
[]
[]
[null,null,null,null,null,null,null,null,"Rad Ventanas: Sol Incidente*FS*FAV*FAR [W]"]
[null,null,null,null,"Mes","Tiempo [hrs]","Tiempo [s]","T° exterior","Difuso","Directo","Qgen Pers [W/m2]","Qgen Ilum [W/m2]","Qgen Equip [W/m2]","TsolH","TsolN","TsolNE","TsolE","TsolSE","TsolS","TsolSO","TsolO","TsolNO","Clima [0, 1 o 2]","N [RAH]","G total [W/m2]"]
[null,"Fila inicial intervalo",{"$f":"TRUNC($C$6/3600,0)+10+32*(E299-1)","v":298},null,"Octubre",0,0,9.6102338709677415,0,0,4.0999999999999996,0,0,5.9043515180265649,9.6102338709677415,9.6102338709677415,9.6102338709677415,9.6102338709677415,9.6102338709677415,9.6102338709677415,9.6102338709677415,9.6102338709677415,0,0.82620000000000016,0]
[null,null,null,null,10,1,3600,8.5124919354838724,0,0,4.0999999999999996,0,0,4.8066095825426958,8.5124919354838724,8.5124919354838724,8.5124919354838724,8.5124919354838724,8.5124919354838724,8.5124919354838724,8.5124919354838724,8.5124919354838724,0,0.82620000000000016,0]
[null,null,null,null,"Tmax Dia",2,7200,7.9181048387096764,0,0,4.0999999999999996,0,0,4.2122224857684998,7.9181048387096764,7.9181048387096764,7.9181048387096764,7.9181048387096764,7.9181048387096764,7.9181048387096764,7.9181048387096764,7.9181048387096764,0,0.82620000000000016,0]
[null,null,null,null,25.075050403225806,3,10800,7.3451370967741934,0,0,4.0999999999999996,0,0,3.6392547438330167,7.3451370967741934,7.3451370967741934,7.3451370967741934,7.3451370967741934,7.3451370967741934,7.3451370967741934,7.3451370967741934,7.3451370967741934,0,0.82620000000000016,0]
[null,null,null,null,"Tmin Dia",4,14400,6.9381693548387098,0,0,4.0999999999999996,0,0,3.2322870018975332,6.9381693548387098,6.9381693548387098,6.9381693548387098,6.9381693548387098,6.9381693548387098,6.9381693548387098,6.9381693548387098,6.9381693548387098,0,0.82620000000000016,0]
[null,null,null,null,20.075050403225806,5,18000,6.8953306451612901,0,0,4.0999999999999996,0,0,3.1894482922201135,6.8953306451612901,6.8953306451612901,6.8953306451612901,6.8953306451612901,6.8953306451612901,6.8953306451612901,6.8953306451612901,6.8953306451612901,0,0.82620000000000016,0]
[null,null,null,null,"Tmax Noche",6,21600,8.4857177419354812,23.01284799502281,0,3.28,0,0,4.8342945920303579,8.5042068315015413,8.5137177224763736,8.517495224221566,8.5107360950355027,8.4999901735367196,8.5107360950355027,8.517495224221566,8.5137177224763736,0,0.82620000000000016,1.3225806451612903]
[null,null,null,null,25.075050403225806,7,25200,10.852556451612905,1068.6942093298399,162.04957078532016,3.9359999999999999,0,0,11.953694971537004,12.484556820870765,13.324066929112579,13.657500558767628,13.060883765490377,12.112359621487991,13.060883765490377,13.657500558767628,13.324066929112579,0,0.82620000000000016,116.74193548387096]
[null,null,null,null,"Tmin Noche",8,28800,13.481782258064516,1928.0276308025209,658.33255035466914,1.968,0,0,22.696013757115747,17.868206019261308,20.124606909802381,21.020796165302425,19.417233980110986,16.867829628436155,19.417233980110986,21.020796165302425,20.124606909802377,0,0.82620000000000016,313.77419354838707]
[null,null,null,null,18.075050403225806,9,32400,16.014620967741934,2823.8448356819454,1161.6033016588583,1.23,0,0,33.737770872865269,23.289852235284634,27.03227184740544,28.518672717044819,25.859037810733163,21.630648748784971,25.859037810733163,28.518672717044819,27.03227184740544,0,0.82620000000000016,520.41935483870964]
[null,null,null,null,"Tsuelo",10,36000,18.231524193548381,3828.5521018061118,1521.112304045801,1.23,0,0,42.896230075901329,27.863437950657698,32.818148202643584,34.786042343511831,31.264865751191081,25.666764841617447,31.264865751191081,34.786042343511831,32.818148202643577,0,0.82620000000000016,689]
[null,null,null,null,14.411962365591398,11,39600,20.003975806451617,4808.0013640333018,1710.4927738712859,1.23,0,0,49.390693074003806,31.239028914959576,37.018403006348514,39.313834188781755,35.206591638986389,28.676740706774325,35.206591638986389,39.313834188781755,37.018403006348507,0,0.82620000000000016,803.67741935483866]
[null,null,null,null,"Infil RAH",12,43200,21.235588709677423,5261.522856227898,756.06595189158838,1.23,0,0,52.56689800759014,33.130837601714951,39.249820092790543,41.680135727783878,37.331542809003196,30.417983850590659,37.331542809003196,41.680135727783878,39.249820092790543,0,3.8262,850.90322580645159]
[null,null,null,null,0,13,46800,21.942427419354839,5314.2840199238044,1969.4580165232878,1.23,0,0,52.452863851992419,33.558987107689312,39.534610315290621,41.907987021539327,37.661275610977853,30.909691761986011,37.661275610977853,41.907987021539327,39.534610315290621,0,3.8262,830.9677419354839]
[null,null,null,null,"Cat Mes",14,50400,22.231588709677418,4654.7694737249794,1856.4305646788689,1.23,0,0,49.939368595825428,32.89663671546586,38.382796997289262,40.561770564943842,36.662907022250565,30.464344986976609,36.662907022250565,40.561770564943842,38.382796997289262,0,3.8262,762.90322580645159]
[null,null,null,null,"v",15,54000,21.92100806451613,3651.1847855517899,1707.2585052392824,1.23,0,0,45.614746204933589,31.223274883264711,36.008412908357869,37.908956957134983,34.508290692497475,29.101781700377767,34.508290692497475,37.908956957134983,36.008412908357869,0,3.8262,665.41935483870964]
[null,null,null,null,null,16,57600,20.860750000000003,2749.7546909174821,1277.149763354317,1.476,0,0,37.695285104364331,27.834293440233086,31.42152314839872,32.846286245659201,30.296940544846986,26.243893470281385,30.296940544846986,32.846286245659201,31.42152314839872,0,3.8262,498.83870967741933]
[null,null,null,null,null,17,61200,19.222169354838712,1887.0535355918705,674.10132748898911,2.46,0,0,28.067140891840609,23.483228069709536,25.67514047998224,26.545716430966088,24.987984438792356,22.511442676792203,24.987984438792356,26.545716430966088,25.675140479982236,0,0.82620000000000016,304.80645161290323]
[null,null,null,null,null,18,64800,17.433653225806449,1075.4296770357,182.39607136099312,2.46,0,0,18.460408444022764,19.040400204437493,19.866919827445393,20.195193942521641,19.607809130571695,18.673962342762771,19.607809130571695,20.195193942521641,19.866919827445393,0,0.82620000000000016,114.93548387096774]
[null,null,null,null,null,19,68400,16.073524193548383,25.819292872464615,0,3.69,1.5,0,12.428742409867169,16.094268050134694,16.104938805862556,16.109176978552284,16.101593565319138,16.089537165588798,16.101593565319138,16.109176978552284,16.104938805862556,0,0.82620000000000016,1.4838709677419355]
[null,null,null,null,null,20,72000,14.708040322580644,0,0,4.4279999999999999,1.5,0,11.002157969639466,14.708040322580644,14.708040322580644,14.708040322580644,14.708040322580644,14.708040322580644,14.708040322580644,14.708040322580644,14.708040322580644,0,0.82620000000000016,0]
[null,null,null,null,null,21,75600,13.347911290322578,0,0,4.92,1.5,0,9.6420289373814008,13.347911290322578,13.347911290322578,13.347911290322578,13.347911290322578,13.347911290322578,13.347911290322578,13.347911290322578,13.347911290322578,0,0.82620000000000016,0]
[null,null,null,null,null,22,79200,11.993137096774193,0,0,4.0999999999999996,0,0,8.2872547438330173,11.993137096774193,11.993137096774193,11.993137096774193,11.993137096774193,11.993137096774193,11.993137096774193,11.993137096774193,11.993137096774193,0,0.82620000000000016,0]
[null,null,null,null,null,23,82800,10.627653225806453,0,0,4.0999999999999996,0,0,6.9217708728652765,10.627653225806453,10.627653225806453,10.627653225806453,10.627653225806453,10.627653225806453,10.627653225806453,10.627653225806453,10.627653225806453,0,0.82620000000000016,0]
[null,null,null,null,null,24,86400,9.6102338709677415,0,0,4.0999999999999996,0,0,5.9043515180265649,9.6102338709677415,9.6102338709677415,9.6102338709677415,9.6102338709677415,9.6102338709677415,9.6102338709677415,9.6102338709677415,9.6102338709677415,0,0.82620000000000016,0]
[null,null,null,null,null,null,"Valor Variable",{"$f":"+INDIRECT(H324&$C298)+((INDIRECT(H324&$C298+1)-INDIRECT(H324&$C298))/(INDIRECT($C$4&$C298+1)-INDIRECT($C$4&$C298)))*($C$6-INDIRECT($C$4&$C298))","v":9.6102338709677415},{"$f":"+INDIRECT(I324&$C298)+((INDIRECT(I324&$C298+1)-INDIRECT(I324&$C298))/(INDIRECT($C$4&$C298+1)-INDIRECT($C$4&$C298)))*($C$6-INDIRECT($C$4&$C298))","v":0},0,4.0999999999999996,0,{"$f":"+INDIRECT(M324&$C298)+((INDIRECT(M324&$C298+1)-INDIRECT(M324&$C298))/(INDIRECT($C$4&$C298+1)-INDIRECT($C$4&$C298)))*($C$6-INDIRECT($C$4&$C298))","v":0},5.9043515180265649,9.6102338709677415,9.6102338709677415,9.6102338709677415,9.6102338709677415,9.6102338709677415,9.6102338709677415,9.6102338709677415,9.6102338709677415,{"$f":"+INDIRECT(W324&$C298)","v":0},0.82620000000000016,0]
[null,null,null,null,null,null,null,{"$f":"MID(ADDRESS(ROW(),COLUMN()),2,1)","v":"H"},{"$f":"MID(ADDRESS(ROW(),COLUMN()),2,1)","v":"I"},"J","K","L","M","N","O","P","Q","R","S","T","U","V","W","X","Y"]
[]
[]
[]
[null,null,null,null,null,null,null,null,"Rad Ventanas: Sol Incidente*FS*FAV*FAR [W]"]
[null,null,null,null,"Mes","Tiempo [hrs]","Tiempo [s]","T° exterior","Difuso","Directo","Qgen Pers [W/m2]","Qgen Ilum [W/m2]","Qgen Equip [W/m2]","TsolH","TsolN","TsolNE","TsolE","TsolSE","TsolS","TsolSO","TsolO","TsolNO","Clima [0, 1 o 2]","N [RAH]","G total [W/m2]"]
[null,"Fila inicial intervalo",{"$f":"TRUNC($C$6/3600,0)+10+32*(E331-1)","v":330},null,"Noviembre",0,0,11.188222222222221,0,0,4.0999999999999996,0,0,7.4823398692810441,11.188222222222221,11.188222222222221,11.188222222222221,11.188222222222221,11.188222222222221,11.188222222222221,11.188222222222221,11.188222222222221,0,0.82620000000000016,0]
[null,null,null,null,11,1,3600,10.192722222222223,0,0,4.0999999999999996,0,0,6.4868398692810461,10.192722222222223,10.192722222222223,10.192722222222223,10.192722222222223,10.192722222222223,10.192722222222223,10.192722222222223,10.192722222222223,0,0.82620000000000016,0]
[null,null,null,null,"Tmax Dia",2,7200,9.6262222222222231,0,0,4.0999999999999996,0,0,5.9203398692810465,9.6262222222222231,9.6262222222222231,9.6262222222222231,9.6262222222222231,9.6262222222222231,9.6262222222222231,9.6262222222222231,9.6262222222222231,0,0.82620000000000016,0]
[null,null,null,null,25.507766666666665,3,10800,9.0872222222222252,0,0,4.0999999999999996,0,0,5.3813398692810486,9.0872222222222252,9.0872222222222252,9.0872222222222252,9.0872222222222252,9.0872222222222252,9.0872222222222252,9.0872222222222252,9.0872222222222252,0,0.82620000000000016,0]
[null,null,null,null,"Tmin Dia",4,14400,8.7077222222222215,0,0,4.0999999999999996,0,0,5.0018398692810448,8.7077222222222215,8.7077222222222215,8.7077222222222215,8.7077222222222215,8.7077222222222215,8.7077222222222215,8.7077222222222215,8.7077222222222215,0,0.82620000000000016,0]
[null,null,null,null,20.507766666666665,5,18000,8.8562222222222218,0,0,4.0999999999999996,0,0,5.1503398692810451,8.8562222222222218,8.8562222222222218,8.8562222222222218,8.8562222222222218,8.8562222222222218,8.8562222222222218,8.8562222222222218,8.8562222222222218,0,0.82620000000000016,0]
[null,null,null,null,"Tmax Noche",6,21600,10.918722222222222,157.17962276925741,0,3.28,0,0,7.5848006535947698,11.007254035086619,11.080160722689085,11.132095187694501,11.110518973654136,11.05018708533132,11.110518973654136,11.132095187694501,11.080160722689085,0,0.82620000000000016,9.0333333333333332]
[null,null,null,null,25.507766666666665,7,25200,13.322222222222223,1746.9558073099756,249.22563917174631,3.9359999999999999,0,0,16.658888888888889,14.998446324831894,16.378830878663074,17.36213619210514,16.953621231805801,15.811322637767564,16.953621231805801,17.36213619210514,16.37883087866307,0,0.82620000000000016,171.03333333333333]
[null,null,null,null,"Tmin Noche",8,28800,15.824722222222221,2261.9945712180956,861.76321765520788,1.968,0,0,27.528447712418298,19.492422085796335,22.512803568131677,24.664346884057245,23.770486533388631,21.271054392428329,23.770486533388631,24.664346884057245,22.512803568131673,0,0.82620000000000016,374.23333333333335]
[null,null,null,null,18.507766666666665,9,32400,18.151222222222223,3307.7320614504611,1376.6805599364279,1.23,0,0,38.33867320261438,23.838166127548504,28.521411949628636,31.857482675880732,30.471509487634606,26.596020513746932,30.471509487634606,31.857482675880732,28.521411949628636,0,0.82620000000000016,580.26666666666665]
[null,null,null,null,"Tsuelo",10,36000,20.224722222222223,4260.0897757940802,1765.750127836445,1.23,0,0,47.206290849673209,27.528760126363135,33.543696367750286,37.82838555074342,36.048308083900196,31.070815983820882,36.048308083900196,37.82838555074342,33.543696367750286,0,0.82620000000000016,745.26666666666665]
[null,null,null,null,16.108888888888888,11,39600,21.682222222222219,4799.4884812383953,2104.2453564991574,1.23,0,0,53.890457516339865,30.230279105653256,37.26967537062044,42.284130024981216,40.200870923209152,34.375615610091913,40.200870923209152,42.284130024981216,37.269675370620433,0,3.8262,872.2]
[null,null,null,null,"Infil RAH",12,43200,22.75472222222222,5796.5060883983715,517.05427411730989,1.23,0,0,54.798251633986929,31.263576826894116,38.270689687756885,43.262147531045152,41.188442472390591,35.389902386574967,41.188442472390591,43.262147531045152,38.270689687756885,0,3.8262,868.2]
[null,null,null,null,0,13,46800,23.337722222222219,6001.8255956320145,1936.6774494001554,1.23,0,0,55.021643790849673,31.760985184936651,38.697612613504788,43.638860752618072,41.586015354770069,35.845803515229633,41.586015354770069,43.638860752618072,38.697612613504788,0,3.8262,859.4666666666667]
[null,null,null,null,"Cat Mes",14,50400,23.453222222222223,5212.4474901376998,1834.5489547246098,1.23,0,0,52.151849673202619,31.165943882427197,37.517434611602852,42.041865550026898,40.162187183683677,34.906188838985031,40.162187183683677,42.041865550026898,37.517434611602852,0,3.8262,786.9666666666667]
[null,null,null,null,"v",15,54000,23.101222222222212,4510.0691758440807,1560.533435840835,1.23,0,0,47.140045751633977,29.704846079199775,35.14298550058809,39.016798325752376,37.407419762608583,32.907239723651465,37.407419762608583,39.016798325752376,35.14298550058809,0,3.8262,673.8]
[null,null,null,null,null,16,57600,22.078222222222223,3409.2318178512737,1222.781706520725,1.476,0,0,39.817045751633984,27.182358916662587,31.385658131057113,34.379842932697898,33.135906518798691,29.65758392412836,33.135906518798691,34.379842932697898,31.385658131057113,0,3.8262,520.79999999999995]
[null,null,null,null,null,17,61200,20.620722222222224,2355.3743471068428,744.38373330468528,2.46,0,0,30.632094771241828,23.885618671546148,26.574288176708649,28.489539258864177,27.693846701227933,25.46891352079173,27.693846701227933,28.489539258864177,26.574288176708649,0,3.8262,333.13333333333333]
[null,null,null,null,null,18,64800,18.860722222222218,1628.636091277029,233.11393502108635,2.46,0,0,21.559153594771235,20.385037494640212,21.640323857566791,22.534516528102884,22.16302348488388,21.1242463966394,22.16302348488388,22.534516528102884,21.640323857566791,0,0.82620000000000016,155.53333333333333]
[null,null,null,null,null,19,68400,17.529722222222219,154.85962833723889,0,3.69,0,0,14.190310457516336,17.616947292461312,17.688777866593629,17.739945771229962,17.718688025293513,17.659246644547419,17.718688025293513,17.739945771229962,17.688777866593629,0,0.82620000000000016,8.9]
[null,null,null,null,null,20,72000,16.242722222222223,0,0,4.4279999999999999,1.5,0,12.536839869281046,16.242722222222223,16.242722222222223,16.242722222222223,16.242722222222223,16.242722222222223,16.242722222222223,16.242722222222223,16.242722222222223,0,0.82620000000000016,0]
[null,null,null,null,null,21,75600,14.928222222222221,0,0,4.92,1.5,0,11.222339869281043,14.928222222222221,14.928222222222221,14.928222222222221,14.928222222222221,14.928222222222221,14.928222222222221,14.928222222222221,14.928222222222221,0,0.82620000000000016,0]
[null,null,null,null,null,22,79200,13.61372222222222,0,0,4.0999999999999996,0,0,9.9078398692810445,13.61372222222222,13.61372222222222,13.61372222222222,13.61372222222222,13.61372222222222,13.61372222222222,13.61372222222222,13.61372222222222,0,0.82620000000000016,0]
[null,null,null,null,null,23,82800,12.310222222222219,0,0,4.0999999999999996,0,0,8.6043398692810413,12.310222222222219,12.310222222222219,12.310222222222219,12.310222222222219,12.310222222222219,12.310222222222219,12.310222222222219,12.310222222222219,0,0.82620000000000016,0]
[null,null,null,null,null,24,86400,11.188222222222221,0,0,4.0999999999999996,0,0,7.4823398692810441,11.188222222222221,11.188222222222221,11.188222222222221,11.188222222222221,11.188222222222221,11.188222222222221,11.188222222222221,11.188222222222221,0,0.82620000000000016,0]
[null,null,null,null,null,null,"Valor Variable",{"$f":"+INDIRECT(H356&$C330)+((INDIRECT(H356&$C330+1)-INDIRECT(H356&$C330))/(INDIRECT($C$4&$C330+1)-INDIRECT($C$4&$C330)))*($C$6-INDIRECT($C$4&$C330))","v":11.188222222222221},{"$f":"+INDIRECT(I356&$C330)+((INDIRECT(I356&$C330+1)-INDIRECT(I356&$C330))/(INDIRECT($C$4&$C330+1)-INDIRECT($C$4&$C330)))*($C$6-INDIRECT($C$4&$C330))","v":0},0,4.0999999999999996,0,{"$f":"+INDIRECT(M356&$C330)+((INDIRECT(M356&$C330+1)-INDIRECT(M356&$C330))/(INDIRECT($C$4&$C330+1)-INDIRECT($C$4&$C330)))*($C$6-INDIRECT($C$4&$C330))","v":0},7.4823398692810441,11.188222222222221,11.188222222222221,11.188222222222221,11.188222222222221,11.188222222222221,11.188222222222221,11.188222222222221,11.188222222222221,{"$f":"+INDIRECT(W356&$C330)","v":0},0.82620000000000016,0]
[null,null,null,null,null,null,null,{"$f":"MID(ADDRESS(ROW(),COLUMN()),2,1)","v":"H"},{"$f":"MID(ADDRESS(ROW(),COLUMN()),2,1)","v":"I"},"J","K","L","M","N","O","P","Q","R","S","T","U","V","W","X","Y"]
[]
[]
[]
[null,null,null,null,null,null,null,null,"Rad Ventanas: Sol Incidente*FS*FAV*FAR [W]"]
[null,null,null,null,"Mes","Tiempo [hrs]","Tiempo [s]","T° exterior","Difuso","Directo","Qgen Pers [W/m2]","Qgen Ilum [W/m2]","Qgen Equip [W/m2]","TsolH","TsolN","TsolNE","TsolE","TsolSE","TsolS","TsolSO","TsolO","TsolNO","Clima [0, 1 o 2]","N [RAH]","G total [W/m2]"]
[null,"Fila inicial intervalo",{"$f":"TRUNC($C$6/3600,0)+10+32*(E363-1)","v":362},null,"Diciembre",0,0,12.951213709677418,0,0,4.0999999999999996,0,0,9.2453313567362407,12.951213709677418,12.951213709677418,12.951213709677418,12.951213709677418,12.951213709677418,12.951213709677418,12.951213709677418,12.951213709677418,0,0.82620000000000016,0]
[null,null,null,null,12,1,3600,11.952794354838709,0,0,4.0999999999999996,0,0,8.246912001897531,11.952794354838709,11.952794354838709,11.952794354838709,11.952794354838709,11.952794354838709,11.952794354838709,11.952794354838709,11.952794354838709,0,0.82620000000000016,0]
[null,null,null,null,"Tmax Dia",2,7200,11.406697580645165,0,0,4.0999999999999996,0,0,7.7008152277039885,11.406697580645165,11.406697580645165,11.406697580645165,11.406697580645165,11.406697580645165,11.406697580645165,11.406697580645165,11.406697580645165,0,0.82620000000000016,0]
[null,null,null,null,25.980643145161288,3,10800,10.866116935483873,0,0,4.0999999999999996,0,0,7.1602345825426967,10.866116935483873,10.866116935483873,10.866116935483873,10.866116935483873,10.866116935483873,10.866116935483873,10.866116935483873,10.866116935483873,0,0.82620000000000016,0]
[null,null,null,null,"Tmin Dia",4,14400,10.468955645161289,0,0,4.0999999999999996,0,0,6.7630732922201124,10.468955645161289,10.468955645161289,10.468955645161289,10.468955645161289,10.468955645161289,10.468955645161289,10.468955645161289,10.468955645161289,0,0.82620000000000016,0]
[null,null,null,null,20.980643145161288,5,18000,10.805439516129036,0,0,4.0999999999999996,0,0,7.0995571631878596,10.805439516129036,10.805439516129036,10.805439516129036,10.805439516129036,10.805439516129036,10.805439516129036,10.805439516129036,10.805439516129036,0,0.82620000000000016,0]
[null,null,null,null,"Tmax Noche",6,21600,12.951213709677416,301.97346881273836,0,3.28,0,0,9.9599423624288406,13.125282797007037,13.239001359946938,13.358190971158205,13.340105319226756,13.265905342894541,13.340105319226756,13.358190971158205,13.239001359946938,0,0.82620000000000016,17.35483870967742]
[null,null,null,null,25.980643145161288,7,25200,15.22385887096774,2029.0596463904258,320.81931161541291,3.9359999999999999,0,0,19.62442813092979,17.19847530214372,18.488483461292823,19.8405544598474,19.635393244721687,18.793678643317385,19.635393244721687,19.8405544598474,18.488483461292823,0,0.82620000000000016,196.87096774193549]
[null,null,null,null,"Tmin Noche",8,28800,17.50753629032258,2965.8509464805006,898.88722719897237,1.968,0,0,30.079642552182161,21.472623028658091,24.062996613841161,26.777994170335724,26.366024533867495,24.675837340649451,26.366024533867495,26.777994170335724,24.062996613841161,0,0.82620000000000016,395.32258064516128]
[null,null,null,null,18.980643145161288,9,32400,19.730536290322576,4142.312639104106,1393.3977014936302,1.23,0,0,40.18063116698292,25.614589119646901,29.458614743485278,33.487578069671329,32.876229248062913,30.368049378959412,32.876229248062913,33.487578069671329,29.458614743485278,0,0.82620000000000016,586.64516129032256]
[null,null,null,null,"Tsuelo",10,36000,21.633600806451607,5070.6846045618558,1880.3003223376006,1.23,0,0,49.296219402277032,29.274521933545152,34.266301826460975,39.498238366173382,38.704352202580267,35.447276661573547,38.704352202580267,39.498238366173382,34.266301826460975,0,3.8262,761.80645161290317]
[null,null,null,null,17.963306451612905,11,39600,23.222245967741937,5830.1085883976084,2165.9171934100041,1.23,0,0,55.624143500948776,32.017588105229699,37.763546125598246,43.785944622191323,42.872114952852094,39.122947375500864,42.872114952852094,43.785944622191323,37.763546125598246,0,3.8262,876.90322580645159]
[null,null,null,null,"Infil RAH",12,43200,24.413729838709681,6510.3908266895023,1024.5203758465475,1.23,0,0,59.709934772296023,33.914084134731354,40.120623472285864,46.625762048487402,45.638682127180459,41.588990853866591,45.638682127180459,46.625762048487402,40.120623472285864,0,3.8262,947.19354838709683]
[null,null,null,null,0,13,46800,25.152891129032263,6445.84259450834,2352.5308708497951,1.23,0,0,60.326894924098681,34.62347896402359,40.810572004569792,47.29532871417014,46.311341506576383,42.274338705051669,46.311341506576383,47.29532871417014,40.810572004569792,0,3.8262,944.22580645161293]
[null,null,null,null,"Cat Mes",14,50400,25.434213709677426,5503.9996936388698,2352.1340870969107,1.23,0,0,58.375390180265669,34.360916533886055,40.19269190844345,46.305036468515667,45.377558519094336,41.572396164064884,45.377558519094336,46.305036468515667,40.19269190844345,0,3.8262,890]
[null,null,null,null,"v",15,54000,25.213568548387098,4876.4786190428822,2016.9840771608128,1.23,0,0,53.303891129032266,32.958672289086849,38.01851422153176,43.321787294348312,42.517076632759043,39.215591440490293,42.517076632759043,43.321787294348312,38.01851422153176,0,3.8262,772.19354838709683]
[null,null,null,null,null,16,57600,24.325471774193549,3909.9390032519241,1552.6148250354604,1.476,0,0,45.464940464895633,30.377446269547747,34.331174373248224,38.475118012108346,37.846322251183153,35.266562851008246,37.846322251183153,38.475118012108346,34.331174373248224,0,3.8262,603.38709677419354]
[null,null,null,null,null,17,61200,22.913342741935484,2803.6384325643644,1019.8665061630836,2.46,0,0,36.084500237191648,27.024349849017572,29.710052564100078,32.524965575346087,32.097834918392579,30.345446629773363,32.097834918392579,32.524965575346087,29.710052564100078,0,3.8262,409.87096774193549]
[null,null,null,null,null,18,64800,21.131633064516134,2011.0983991747983,363.71844014375301,2.46,0,0,25.837705170777991,23.180665648267972,24.519289549937852,25.922315214995386,25.709422215586713,24.835986434709529,25.709422215586713,25.922315214995386,24.519289549937852,0,3.8262,204.29032258064515]
[null,null,null,null,null,19,68400,19.675375000000003,349.12174275376071,0,3.69,0,0,16.795678605313096,19.876622160444285,20.008096038043949,20.145895179630209,20.124985745612808,20.039200642864412,20.124985745612808,20.145895179630209,20.008096038043949,0,0.82620000000000016,20.06451612903226]
[null,null,null,null,null,20,72000,18.213600806451616,0,0,4.4279999999999999,1.5,0,14.507718453510439,18.213600806451616,18.213600806451616,18.213600806451616,18.213600806451616,18.213600806451616,18.213600806451616,18.213600806451616,18.213600806451616,0,0.82620000000000016,0]
[null,null,null,null,null,21,75600,16.773891129032254,0,0,4.92,1.5,0,13.068008776091077,16.773891129032254,16.773891129032254,16.773891129032254,16.773891129032254,16.773891129032254,16.773891129032254,16.773891129032254,16.773891129032254,0,0.82620000000000016,0]
[null,null,null,null,null,22,79200,15.306600806451609,0,0,4.0999999999999996,0,0,11.600718453510432,15.306600806451609,15.306600806451609,15.306600806451609,15.306600806451609,15.306600806451609,15.306600806451609,15.306600806451609,15.306600806451609,0,3.8262,0]
[null,null,null,null,null,23,82800,13.844826612903221,0,0,4.0999999999999996,0,0,10.138944259962045,13.844826612903221,13.844826612903221,13.844826612903221,13.844826612903221,13.844826612903221,13.844826612903221,13.844826612903221,13.844826612903221,0,0.82620000000000016,0]
[null,null,null,null,null,24,86400,12.951213709677418,0,0,4.0999999999999996,0,0,9.2453313567362407,12.951213709677418,12.951213709677418,12.951213709677418,12.951213709677418,12.951213709677418,12.951213709677418,12.951213709677418,12.951213709677418,0,0.82620000000000016,0]
[null,null,null,null,null,null,"Valor Variable",{"$f":"+INDIRECT(H388&$C362)+((INDIRECT(H388&$C362+1)-INDIRECT(H388&$C362))/(INDIRECT($C$4&$C362+1)-INDIRECT($C$4&$C362)))*($C$6-INDIRECT($C$4&$C362))","v":12.951213709677418},{"$f":"+INDIRECT(I388&$C362)+((INDIRECT(I388&$C362+1)-INDIRECT(I388&$C362))/(INDIRECT($C$4&$C362+1)-INDIRECT($C$4&$C362)))*($C$6-INDIRECT($C$4&$C362))","v":0},0,4.0999999999999996,0,{"$f":"+INDIRECT(M388&$C362)+((INDIRECT(M388&$C362+1)-INDIRECT(M388&$C362))/(INDIRECT($C$4&$C362+1)-INDIRECT($C$4&$C362)))*($C$6-INDIRECT($C$4&$C362))","v":0},9.2453313567362407,12.951213709677418,12.951213709677418,12.951213709677418,12.951213709677418,12.951213709677418,12.951213709677418,12.951213709677418,12.951213709677418,{"$f":"+INDIRECT(W388&$C362)","v":0},0.82620000000000016,0]
[null,null,null,null,null,null,null,{"$f":"MID(ADDRESS(ROW(),COLUMN()),2,1)","v":"H"},{"$f":"MID(ADDRESS(ROW(),COLUMN()),2,1)","v":"I"},"J","K","L","M","N","O","P","Q","R","S","T","U","V","W","X","Y"]

{"sheet":"SA","index":1,"n_rows":87,"n_cols":19,"rows_kept":87,"cut":false,"hidden":true,"merged":[[61,5,61,6],[61,7,61,8],[61,9,61,10],[61,11,61,12],[33,5,33,6],[33,7,33,8],[33,9,33,10],[33,11,33,12]]}
[]
[null,null,null,"Serie de Amplificacion"]
[null,null,null,"Horiz","N","NE","E","SE","S","SO","O","NO","Piso Vent","Piso Terreno"]
[null,null,1,{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",H64,I64),IF($B$26=\"v\",H36,I36))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F64,G64),IF($B$26=\"v\",F36,G36))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F64,G64),IF($B$26=\"v\",F36,G36))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F64,G64),IF($B$26=\"v\",F36,G36))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F64,G64),IF($B$26=\"v\",F36,G36))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F64,G64),IF($B$26=\"v\",F36,G36))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F64,G64),IF($B$26=\"v\",F36,G36))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F64,G64),IF($B$26=\"v\",F36,G36))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F64,G64),IF($B$26=\"v\",F36,G36))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",J64,K64),IF($B$26=\"v\",J36,K36))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",L64,M64),IF($B$26=\"v\",L36,M36))","v":0}]
[null,null,2,{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",H65,I65),IF($B$26=\"v\",H37,I37))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F65,G65),IF($B$26=\"v\",F37,G37))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F65,G65),IF($B$26=\"v\",F37,G37))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F65,G65),IF($B$26=\"v\",F37,G37))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F65,G65),IF($B$26=\"v\",F37,G37))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F65,G65),IF($B$26=\"v\",F37,G37))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F65,G65),IF($B$26=\"v\",F37,G37))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F65,G65),IF($B$26=\"v\",F37,G37))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F65,G65),IF($B$26=\"v\",F37,G37))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",J65,K65),IF($B$26=\"v\",J37,K37))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",L65,M65),IF($B$26=\"v\",L37,M37))","v":0}]
[null,null,3,{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",H66,I66),IF($B$26=\"v\",H38,I38))","v":58.00200000000001},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F66,G66),IF($B$26=\"v\",F38,G38))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F66,G66),IF($B$26=\"v\",F38,G38))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F66,G66),IF($B$26=\"v\",F38,G38))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F66,G66),IF($B$26=\"v\",F38,G38))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F66,G66),IF($B$26=\"v\",F38,G38))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F66,G66),IF($B$26=\"v\",F38,G38))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F66,G66),IF($B$26=\"v\",F38,G38))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F66,G66),IF($B$26=\"v\",F38,G38))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",J66,K66),IF($B$26=\"v\",J38,K38))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",L66,M66),IF($B$26=\"v\",L38,M38))","v":0}]
[null,null,4,{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",H67,I67),IF($B$26=\"v\",H39,I39))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F67,G67),IF($B$26=\"v\",F39,G39))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F67,G67),IF($B$26=\"v\",F39,G39))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F67,G67),IF($B$26=\"v\",F39,G39))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F67,G67),IF($B$26=\"v\",F39,G39))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F67,G67),IF($B$26=\"v\",F39,G39))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F67,G67),IF($B$26=\"v\",F39,G39))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F67,G67),IF($B$26=\"v\",F39,G39))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F67,G67),IF($B$26=\"v\",F39,G39))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",J67,K67),IF($B$26=\"v\",J39,K39))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",L67,M67),IF($B$26=\"v\",L39,M39))","v":0}]
[null,null,5,{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",H68,I68),IF($B$26=\"v\",H40,I40))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F68,G68),IF($B$26=\"v\",F40,G40))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F68,G68),IF($B$26=\"v\",F40,G40))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F68,G68),IF($B$26=\"v\",F40,G40))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F68,G68),IF($B$26=\"v\",F40,G40))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F68,G68),IF($B$26=\"v\",F40,G40))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F68,G68),IF($B$26=\"v\",F40,G40))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F68,G68),IF($B$26=\"v\",F40,G40))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F68,G68),IF($B$26=\"v\",F40,G40))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",J68,K68),IF($B$26=\"v\",J40,K40))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",L68,M68),IF($B$26=\"v\",L40,M40))","v":0}]
[null,null,6,{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",H69,I69),IF($B$26=\"v\",H41,I41))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F69,G69),IF($B$26=\"v\",F41,G41))","v":56.550000000000239},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F69,G69),IF($B$26=\"v\",F41,G41))","v":56.550000000000239},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F69,G69),IF($B$26=\"v\",F41,G41))","v":56.550000000000239},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F69,G69),IF($B$26=\"v\",F41,G41))","v":56.550000000000239},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F69,G69),IF($B$26=\"v\",F41,G41))","v":56.550000000000239},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F69,G69),IF($B$26=\"v\",F41,G41))","v":56.550000000000239},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F69,G69),IF($B$26=\"v\",F41,G41))","v":56.550000000000239},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F69,G69),IF($B$26=\"v\",F41,G41))","v":56.550000000000239},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",J69,K69),IF($B$26=\"v\",J41,K41))","v":75.400000000000318},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",L69,M69),IF($B$26=\"v\",L41,M41))","v":0}]
[null,null,7,{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",H70,I70),IF($B$26=\"v\",H42,I42))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F70,G70),IF($B$26=\"v\",F42,G42))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F70,G70),IF($B$26=\"v\",F42,G42))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F70,G70),IF($B$26=\"v\",F42,G42))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F70,G70),IF($B$26=\"v\",F42,G42))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F70,G70),IF($B$26=\"v\",F42,G42))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F70,G70),IF($B$26=\"v\",F42,G42))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F70,G70),IF($B$26=\"v\",F42,G42))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F70,G70),IF($B$26=\"v\",F42,G42))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",J70,K70),IF($B$26=\"v\",J42,K42))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",L70,M70),IF($B$26=\"v\",L42,M42))","v":0}]
[null,null,8,{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",H71,I71),IF($B$26=\"v\",H43,I43))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F71,G71),IF($B$26=\"v\",F43,G43))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F71,G71),IF($B$26=\"v\",F43,G43))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F71,G71),IF($B$26=\"v\",F43,G43))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F71,G71),IF($B$26=\"v\",F43,G43))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F71,G71),IF($B$26=\"v\",F43,G43))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F71,G71),IF($B$26=\"v\",F43,G43))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F71,G71),IF($B$26=\"v\",F43,G43))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F71,G71),IF($B$26=\"v\",F43,G43))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",J71,K71),IF($B$26=\"v\",J43,K43))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",L71,M71),IF($B$26=\"v\",L43,M43))","v":0}]
[null,null,9,{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",H72,I72),IF($B$26=\"v\",H44,I44))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F72,G72),IF($B$26=\"v\",F44,G44))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F72,G72),IF($B$26=\"v\",F44,G44))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F72,G72),IF($B$26=\"v\",F44,G44))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F72,G72),IF($B$26=\"v\",F44,G44))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F72,G72),IF($B$26=\"v\",F44,G44))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F72,G72),IF($B$26=\"v\",F44,G44))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F72,G72),IF($B$26=\"v\",F44,G44))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F72,G72),IF($B$26=\"v\",F44,G44))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",J72,K72),IF($B$26=\"v\",J44,K44))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",L72,M72),IF($B$26=\"v\",L44,M44))","v":0}]
[null,null,10,{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",H73,I73),IF($B$26=\"v\",H45,I45))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F73,G73),IF($B$26=\"v\",F45,G45))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F73,G73),IF($B$26=\"v\",F45,G45))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F73,G73),IF($B$26=\"v\",F45,G45))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F73,G73),IF($B$26=\"v\",F45,G45))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F73,G73),IF($B$26=\"v\",F45,G45))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F73,G73),IF($B$26=\"v\",F45,G45))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F73,G73),IF($B$26=\"v\",F45,G45))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F73,G73),IF($B$26=\"v\",F45,G45))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",J73,K73),IF($B$26=\"v\",J45,K45))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",L73,M73),IF($B$26=\"v\",L45,M45))","v":0}]
[null,null,11,{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",H74,I74),IF($B$26=\"v\",H46,I46))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F74,G74),IF($B$26=\"v\",F46,G46))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F74,G74),IF($B$26=\"v\",F46,G46))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F74,G74),IF($B$26=\"v\",F46,G46))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F74,G74),IF($B$26=\"v\",F46,G46))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F74,G74),IF($B$26=\"v\",F46,G46))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F74,G74),IF($B$26=\"v\",F46,G46))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F74,G74),IF($B$26=\"v\",F46,G46))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F74,G74),IF($B$26=\"v\",F46,G46))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",J74,K74),IF($B$26=\"v\",J46,K46))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",L74,M74),IF($B$26=\"v\",L46,M46))","v":0}]
[null,null,12,{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",H75,I75),IF($B$26=\"v\",H47,I47))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F75,G75),IF($B$26=\"v\",F47,G47))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F75,G75),IF($B$26=\"v\",F47,G47))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F75,G75),IF($B$26=\"v\",F47,G47))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F75,G75),IF($B$26=\"v\",F47,G47))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F75,G75),IF($B$26=\"v\",F47,G47))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F75,G75),IF($B$26=\"v\",F47,G47))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F75,G75),IF($B$26=\"v\",F47,G47))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F75,G75),IF($B$26=\"v\",F47,G47))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",J75,K75),IF($B$26=\"v\",J47,K47))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",L75,M75),IF($B$26=\"v\",L47,M47))","v":0}]
[null,null,13,{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",H76,I76),IF($B$26=\"v\",H48,I48))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F76,G76),IF($B$26=\"v\",F48,G48))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F76,G76),IF($B$26=\"v\",F48,G48))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F76,G76),IF($B$26=\"v\",F48,G48))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F76,G76),IF($B$26=\"v\",F48,G48))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F76,G76),IF($B$26=\"v\",F48,G48))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F76,G76),IF($B$26=\"v\",F48,G48))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F76,G76),IF($B$26=\"v\",F48,G48))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F76,G76),IF($B$26=\"v\",F48,G48))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",J76,K76),IF($B$26=\"v\",J48,K48))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",L76,M76),IF($B$26=\"v\",L48,M48))","v":0}]
[null,null,14,{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",H77,I77),IF($B$26=\"v\",H49,I49))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F77,G77),IF($B$26=\"v\",F49,G49))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F77,G77),IF($B$26=\"v\",F49,G49))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F77,G77),IF($B$26=\"v\",F49,G49))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F77,G77),IF($B$26=\"v\",F49,G49))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F77,G77),IF($B$26=\"v\",F49,G49))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F77,G77),IF($B$26=\"v\",F49,G49))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F77,G77),IF($B$26=\"v\",F49,G49))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F77,G77),IF($B$26=\"v\",F49,G49))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",J77,K77),IF($B$26=\"v\",J49,K49))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",L77,M77),IF($B$26=\"v\",L49,M49))","v":0}]
[null,null,15,{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",H78,I78),IF($B$26=\"v\",H50,I50))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F78,G78),IF($B$26=\"v\",F50,G50))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F78,G78),IF($B$26=\"v\",F50,G50))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F78,G78),IF($B$26=\"v\",F50,G50))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F78,G78),IF($B$26=\"v\",F50,G50))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F78,G78),IF($B$26=\"v\",F50,G50))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F78,G78),IF($B$26=\"v\",F50,G50))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F78,G78),IF($B$26=\"v\",F50,G50))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F78,G78),IF($B$26=\"v\",F50,G50))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",J78,K78),IF($B$26=\"v\",J50,K50))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",L78,M78),IF($B$26=\"v\",L50,M50))","v":0}]
[null,null,16,{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",H79,I79),IF($B$26=\"v\",H51,I51))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F79,G79),IF($B$26=\"v\",F51,G51))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F79,G79),IF($B$26=\"v\",F51,G51))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F79,G79),IF($B$26=\"v\",F51,G51))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F79,G79),IF($B$26=\"v\",F51,G51))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F79,G79),IF($B$26=\"v\",F51,G51))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F79,G79),IF($B$26=\"v\",F51,G51))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F79,G79),IF($B$26=\"v\",F51,G51))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F79,G79),IF($B$26=\"v\",F51,G51))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",J79,K79),IF($B$26=\"v\",J51,K51))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",L79,M79),IF($B$26=\"v\",L51,M51))","v":0}]
[null,null,17,{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",H80,I80),IF($B$26=\"v\",H52,I52))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F80,G80),IF($B$26=\"v\",F52,G52))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F80,G80),IF($B$26=\"v\",F52,G52))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F80,G80),IF($B$26=\"v\",F52,G52))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F80,G80),IF($B$26=\"v\",F52,G52))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F80,G80),IF($B$26=\"v\",F52,G52))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F80,G80),IF($B$26=\"v\",F52,G52))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F80,G80),IF($B$26=\"v\",F52,G52))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F80,G80),IF($B$26=\"v\",F52,G52))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",J80,K80),IF($B$26=\"v\",J52,K52))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",L80,M80),IF($B$26=\"v\",L52,M52))","v":0}]
[null,null,18,{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",H81,I81),IF($B$26=\"v\",H53,I53))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F81,G81),IF($B$26=\"v\",F53,G53))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F81,G81),IF($B$26=\"v\",F53,G53))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F81,G81),IF($B$26=\"v\",F53,G53))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F81,G81),IF($B$26=\"v\",F53,G53))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F81,G81),IF($B$26=\"v\",F53,G53))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F81,G81),IF($B$26=\"v\",F53,G53))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F81,G81),IF($B$26=\"v\",F53,G53))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F81,G81),IF($B$26=\"v\",F53,G53))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",J81,K81),IF($B$26=\"v\",J53,K53))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",L81,M81),IF($B$26=\"v\",L53,M53))","v":0}]
[null,null,19,{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",H82,I82),IF($B$26=\"v\",H54,I54))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F82,G82),IF($B$26=\"v\",F54,G54))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F82,G82),IF($B$26=\"v\",F54,G54))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F82,G82),IF($B$26=\"v\",F54,G54))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F82,G82),IF($B$26=\"v\",F54,G54))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F82,G82),IF($B$26=\"v\",F54,G54))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F82,G82),IF($B$26=\"v\",F54,G54))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F82,G82),IF($B$26=\"v\",F54,G54))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F82,G82),IF($B$26=\"v\",F54,G54))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",J82,K82),IF($B$26=\"v\",J54,K54))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",L82,M82),IF($B$26=\"v\",L54,M54))","v":0}]
[null,null,20,{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",H83,I83),IF($B$26=\"v\",H55,I55))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F83,G83),IF($B$26=\"v\",F55,G55))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F83,G83),IF($B$26=\"v\",F55,G55))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F83,G83),IF($B$26=\"v\",F55,G55))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F83,G83),IF($B$26=\"v\",F55,G55))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F83,G83),IF($B$26=\"v\",F55,G55))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F83,G83),IF($B$26=\"v\",F55,G55))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F83,G83),IF($B$26=\"v\",F55,G55))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F83,G83),IF($B$26=\"v\",F55,G55))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",J83,K83),IF($B$26=\"v\",J55,K55))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",L83,M83),IF($B$26=\"v\",L55,M55))","v":0}]
[null,null,21,{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",H84,I84),IF($B$26=\"v\",H56,I56))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F84,G84),IF($B$26=\"v\",F56,G56))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F84,G84),IF($B$26=\"v\",F56,G56))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F84,G84),IF($B$26=\"v\",F56,G56))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F84,G84),IF($B$26=\"v\",F56,G56))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F84,G84),IF($B$26=\"v\",F56,G56))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F84,G84),IF($B$26=\"v\",F56,G56))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F84,G84),IF($B$26=\"v\",F56,G56))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F84,G84),IF($B$26=\"v\",F56,G56))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",J84,K84),IF($B$26=\"v\",J56,K56))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",L84,M84),IF($B$26=\"v\",L56,M56))","v":0}]
[null,"Cat. Mes",22,{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",H85,I85),IF($B$26=\"v\",H57,I57))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F85,G85),IF($B$26=\"v\",F57,G57))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F85,G85),IF($B$26=\"v\",F57,G57))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F85,G85),IF($B$26=\"v\",F57,G57))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F85,G85),IF($B$26=\"v\",F57,G57))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F85,G85),IF($B$26=\"v\",F57,G57))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F85,G85),IF($B$26=\"v\",F57,G57))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F85,G85),IF($B$26=\"v\",F57,G57))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F85,G85),IF($B$26=\"v\",F57,G57))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",J85,K85),IF($B$26=\"v\",J57,K57))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",L85,M85),IF($B$26=\"v\",L57,M57))","v":0}]
[null,{"$f":"+Datos!AF3","v":0},23,{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",H86,I86),IF($B$26=\"v\",H58,I58))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F86,G86),IF($B$26=\"v\",F58,G58))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F86,G86),IF($B$26=\"v\",F58,G58))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F86,G86),IF($B$26=\"v\",F58,G58))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F86,G86),IF($B$26=\"v\",F58,G58))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F86,G86),IF($B$26=\"v\",F58,G58))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F86,G86),IF($B$26=\"v\",F58,G58))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F86,G86),IF($B$26=\"v\",F58,G58))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F86,G86),IF($B$26=\"v\",F58,G58))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",J86,K86),IF($B$26=\"v\",J58,K58))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",L86,M86),IF($B$26=\"v\",L58,M58))","v":0}]
[null,null,24,{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",H87,I87),IF($B$26=\"v\",H59,I59))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F87,G87),IF($B$26=\"v\",F59,G59))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F87,G87),IF($B$26=\"v\",F59,G59))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F87,G87),IF($B$26=\"v\",F59,G59))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F87,G87),IF($B$26=\"v\",F59,G59))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F87,G87),IF($B$26=\"v\",F59,G59))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F87,G87),IF($B$26=\"v\",F59,G59))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F87,G87),IF($B$26=\"v\",F59,G59))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",F87,G87),IF($B$26=\"v\",F59,G59))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",J87,K87),IF($B$26=\"v\",J59,K59))","v":0},{"$f":"IF(Calculo!$C$6=\"Si\",IF($B$26=\"v\",L87,M87),IF($B$26=\"v\",L59,M59))","v":0}]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+COLUMN(R33)","v":18}]
[null,null,null,null,"T° Libre",null,null,null,null,null,null,null,null,null,null,{"$f":"+COLUMN(P34)","v":16},null,null,"Espesor de calculo"]
[null,null,null,null,null,"Muros",null,"Techos",null,"Pisos_v",null,"Pisos_t",null,null,null,"e Eq H.A",6.9761068381736271,6.9761068381736271,{"$f":"+IF($B$26=\"v\",Q34,R34)","v":6.9761068381736271}]
[null,null,null,null,null,"SA Verano ","SA Invierno ","SA Verano ","SA Invierno ","SA Verano ","SA Invierno ","SA Verano ","SA Invierno ",null,null,"Área eq H.A",242.28730157199226]
[null,null,null,null,1,0,0,0,0,0,0,0,0]
[null,null,null,null,{"$f":"+E36+1","v":2},0,0,0,0,0,0,0,0,null,null,"Amortiguamiento","CTm","fi"]
[null,null,null,null,{"$f":"+E37+1","v":3},0,0,-12.177999999999997,58.00200000000001,0,0,0,0,null,null,0.36885518843197418,4.1759599339544469,1.8540652651353393]
[null,null,null,null,4,0,0,0,0,0,0,0,0]
[null,null,null,null,5,0,0,0,0,0,0,0,0,null,null,"Participación de Masa"]
[null,null,null,null,6,-13.619999999999987,56.550000000000239,0,0,-18.159999999999982,75.400000000000318,0,0,null,null,"Techo",3.1511166209626559E-2]
[null,null,null,null,7,0,0,0,0,0,0,0,0,null,null,"Muros",0.36513234640325148]
[null,null,null,null,8,0,0,0,0,0,0,0,0,null,null,"Piso v",0.47331057816908467]
[null,null,null,null,9,0,0,0,0,0,0,0,0,null,null,"Piso t",0]
[null,null,null,null,10,0,0,0,0,0,0,0,0,null,null,"Masa ad",0.13004590921803741]
[null,null,null,null,11,0,0,0,0,0,0,0,0]
[null,null,null,null,12,0,0,0,0,0,0,0,0,null,null,"dpm",{"$f":"+IF(S34>=7,5,3)","v":3}]
[null,null,null,null,13,0,0,0,0,0,0,0,0]
[null,null,null,null,14,0,0,0,0,0,0,0,0]
[null,null,null,null,15,0,0,0,0,0,0,0,0]
[null,null,null,null,16,0,0,0,0,0,0,0,0]
[null,null,null,null,17,0,0,0,0,0,0,0,0]
[null,null,null,null,18,0,0,0,0,0,0,0,0]
[null,null,null,null,19,0,0,0,0,0,0,0,0]
[null,null,null,null,20,0,0,0,0,0,0,0,0]
[null,null,null,null,21,0,0,0,0,0,0,0,0]
[null,null,null,null,22,0,0,0,0,0,0,0,0]
[null,null,null,null,23,0,0,0,0,0,0,0,0]
[null,null,null,null,24,0,0,0,0,0,0,0,0]
[]
[null,null,null,null,"Con Clima"]
[null,null,null,null,null,"Muros",null,"Techos",null,"Pisos_v",null,"Pisos_t"]
[null,null,null,null,null,"SA Verano ","SA Invierno ","SA Verano ","SA Invierno ","SA Verano ","SA Invierno ","SA Verano ","SA Invierno "]
[null,null,null,null,1,0,0,0,0,0,0,0,0]
[null,null,null,null,{"$f":"+E64+1","v":2},0,0,0,0,0,0,0,0]
[null,null,null,null,{"$f":"+E65+1","v":3},0,0,-12.177999999999997,58.00200000000001,0,0,0,0]
[null,null,null,null,4,0,0,0,0,0,0,0,0]
[null,null,null,null,5,0,0,0,0,0,0,0,0]
[null,null,null,null,6,-13.619999999999987,56.550000000000239,0,0,-18.159999999999982,75.400000000000318,0,0]
[null,null,null,null,7,0,0,0,0,0,0,0,0]
[null,null,null,null,8,0,0,0,0,0,0,0,0]
[null,null,null,null,9,0,0,0,0,0,0,0,0]
[null,null,null,null,10,0,0,0,0,0,0,0,0]
[null,null,null,null,11,0,0,0,0,0,0,0,0]
[null,null,null,null,12,0,0,0,0,0,0,0,0]
[null,null,null,null,13,0,0,0,0,0,0,0,0]
[null,null,null,null,14,0,0,0,0,0,0,0,0]
[null,null,null,null,15,0,0,0,0,0,0,0,0]
[null,null,null,null,16,0,0,0,0,0,0,0,0]
[null,null,null,null,17,0,0,0,0,0,0,0,0]
[null,null,null,null,18,0,0,0,0,0,0,0,0]
[null,null,null,null,19,0,0,0,0,0,0,0,0]
[null,null,null,null,20,0,0,0,0,0,0,0,0]
[null,null,null,null,21,0,0,0,0,0,0,0,0]
[null,null,null,null,22,0,0,0,0,0,0,0,0]
[null,null,null,null,23,0,0,0,0,0,0,0,0]
[null,null,null,null,24,0,0,0,0,0,0,0,0]

{"sheet":"CEV-CEVE","index":2,"n_rows":239,"n_cols":39,"rows_kept":239,"cut":false,"hidden":true,"merged":[]}
[null,null,"CALIFICACIÓN ENERGÉTICA EN VIVIENDAS EN CHILE"]
[]
[null,null,null,"1.- Características de la vivienda"]
[]
[null,null,null,"1.1.- Datos generales e identificación del proyecto"]
[]
[null,1,"Tipo de Calificación",null,"Calificación",null,"Vivienda nueva"]
[null,2,"Región",null,"I_Región_de_Tarapacá"]
[null,3,"Comuna",null,"Huara",null,null,null,"Tiene las siguientes Zonas Térmicas",null,null,"A","B","H"]
[null,4,"Zona Térmica Proyecto",null,"B",null,null,null,null,null,null,1,1,5,1,null,null,null,null,null,null,null,null,null,null,null,null,"Puertas"]
[null,5,"Dormitorios de la vivienda",null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nombre","Abreviatura","U puerta opaca [W/m2K]","Vidrio","% Vidrio","U Marco [W/m2K]","% Marco","U ponderado","U ponderado opaco","U vidrio [W/m2K]"]
[null,5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Madera Solida","MS",1.91,"VM",0,1.25,8.7800000000000003E-2,1.852052,1.852052,5.8]
[null,6,"Identificación de la vivienda a evaluar",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Madera con hasta 50% zona vidriada","MS < 50% Vidrio",1.91,"VM",0.4,1.25,8.7800000000000003E-2,3.4080519999999996,1.8134199999999998,5.8]
[null,7,"Nombre del proyecto",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Madera con hasta 100% zona vidriada","MS < 100% Vidrio",1.91,"VM",0.85,1.25,8.7800000000000003E-2,5.1585519999999994,1.5236799999999999,5.8]
[null,8,"Dirección de la vivienda",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Liviana de madera","ML",2.63,"VM",0,1.25,8.7800000000000003E-2,2.5088360000000001,2.5088360000000001,5.8]
[null,9,"Tipo de vivienda",null,"Casa Pareada o  continua",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Liviana madera con hasta 50% zona vidriada","ML < 50% Vidrio",2.5299999999999998,"VM",0.45,1.25,8.7800000000000003E-2,3.889116,2.3256654545454545,5.8]
[null,9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Liviana madera con hasta 100% zona vidriada","ML < 100% Vidrio",2.1800000000000002,"VM",0.85,1.25,8.7800000000000003E-2,5.1753459999999993,1.6356400000000002,5.8]
[null,9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario Puerta 1","Abr. Puerta 1",null,null,null,null,null,0,0,0]
[null,10,"Rol vivienda",null,"222-02",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario Puerta 2","Abr. Puerta 2",null,null,null,null,null,0,0,0]
[null,11,"Evaluador energético ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario Puerta 3","Abr. Puerta 3",null,null,null,null,null,0,0,0]
[null,12,"Rol registro de Evaluadores:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario Puerta 4","Abr. Puerta 4",null,null,null,null,null,0,0,0]
[null,13,"RUT Evaluador",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario Puerta 5","Abr. Puerta 5",null,null,null,null,null,0,0,0]
[null,13,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario Puerta 6","Abr. Puerta 6",null,null,null,null,null,0,0,0]
[null,14,"Versión Planilla",null,"01.PBTD Datos de Arquitectura v1.40"]
[null,15,"Caso interno Evaluador",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vidrios"]
[null,16,"Iteración Evaluador",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nombre","Abreviatura","U vidrio [W/m2K]","FS Vidrio"]
[null,16,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vidrio Monolítico (VM). Sin espaciador","VM",5.8,0.87]
[null,17,"Solicitado por:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DVH con espaciador de 6mm","DVH con 6mm",3.28,0.77429999999999999]
[null,18,"RUT Mandante",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DVH con espaciador de 9mm","DVH con 9mm",3.01,0.77429999999999999]
[null,18,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DVH con espaciador de 12mm","DVH con 12mm",2.85,0.77429999999999999]
[null,18,null,"1.2.- Descripción general de los elementos de la envolvente  (esto sólo se utiliza en la confección del certificado)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DVH con espaciador de 15mm o mayor","DVH con 15mm o +",2.8,0.77429999999999999]
[null,18,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario vidrio 1","Abr. Vidrio 1"]
[null,19,"Muro principal",null,"Muro Definido por usuario Muro 1 con aislación por Exterior, de materialidad Pesado, con U= 0,21 [W/m2K], espesor solido15 [cm] y espesor aislante de 16 [cm]",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario vidrio 2","Abr. Vidrio 2"]
[null,20,"Muro secundario",null,"Muro Adiabatico espesor solido 20 [cm]",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario vidrio 3","Abr. Vidrio 3"]
[null,21,"Piso principal",null,"Piso Definido por usuario Piso 2 con aislación por Exterior, con U del piso ventilado = 0,39 [W/m2K],  con aislación bajo piso de conductividad 0,04[ mK/W] , con refuerzo vertical de sobrecimiento con R100 = 125 [100*m2K/W]",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "," ",null,"Definido por usuario vidrio 4","Abr. Vidrio 4"]
[null,22,"Techo principal",null,"Techo Definido por usuario Techo 1 con aislación por Exterior con U= 0,14 [W/m2K] y espesor aislante de 28 [cm]",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario vidrio 5","Abr. Vidrio 5"]
[null,23,"Techo secundario",null,"Techo Definido por usuario Techo 2 con aislación por Exterior con U= 0,24 [W/m2K] y espesor aislante de 14 [cm]",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario vidrio 6","Abr. Vidrio 6"]
[null,24,"Ventana principal: Vidrio y Marco ",null,"Vidrio Definido por usuario vidrio 1 con U= 1,1 [W/m2K] y factor solar de 0,7",null,null,null,null,null,null,null,null,null,"Marco  con U= 5,8 [W/m2K] y factor Marco de 0,8",null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario vidrio 7","Abr. Vidrio 7"]
[null,25,"Ventana secundaria: Vidrio y Marco ",null,"Vidrio Definido por usuario vidrio 1 con U= 1,1 [W/m2K] y factor solar de 0,7",null,null,null,null,null,null,null,null,null,"Marco  con U= 1,8 [W/m2K] y factor Marco de 0,8",null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario vidrio 8","Abr. Vidrio 8"]
[null,26,"Puerta principal",null,"Puerta Definido por usuario Puerta 1 con U= 1,7 [W/m2K] y  0 % de vidrio",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario vidrio 9","Abr. Vidrio 9"]
[null,26,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario vidrio 10","Abr. Vidrio 10"]
[null,26,null,"1.3.- Descripción general de los sistemas de calefacción y agua caliente sanitaria",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario vidrio 11","Abr. Vidrio 11"]
[null,26]
[null,27,"Sistema de calefacción",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Marcos Ventana"]
[null,28,"Sistema de agua caliente",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nombre tipo de Marcos","Abreviatura","Ufr [W/m2K]","FM"]
[null,28,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Madera","Madera",2.6,0.95]
[null,28,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Policloruro de Vinilo","PVC",2.8,0.85]
[null,28,null,"2.- Dimensiones de la vivienda",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Metal sin Ruptura de Puente Térmico","Sin RPT",5.8,0.8]
[null,28,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Metal con Ruptura de Puente Térmico","Con RPT",3.3,0.8]
[null,28,null,"Area [m²]","Altura [m]","Volumen [m3]",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario Marco 1","Abr. Marco 1"]
[null,28,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario Marco 2","Abr. Marco 2"]
[null,29,"Piso 1",80,2.5,200,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario Marco 3","Abr. Marco 3"]
[null,30,"Piso 2",null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario Marco 4","Abr. Marco 4"]
[null,31,"Piso 3+4+..",null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario Marco 5","Abr. Marco 5"]
[null,31,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario Marco 6","Abr. Marco 6"]
[null,32,"Total ",80,null,200,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario Marco 7","Abr. Marco 7"]
[null,32,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario Marco 8","Abr. Marco 8"]
[null,32]
[null,32,null,"3.- Características térmicas de la envolvente",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Muros transmitancia"]
[null,32,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nombre","Abreviatura","Tipología/materialidad","U  [W/m2K]","espesor muro solido [cm]","espesor aislante [cm]","Posición Aislación"]
[null,32,null,"3.1.- Area y coeficiente de transferencia de calor por elemento constructivo",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Adiabatico","Muro Adiabatico","Pesado",null,20,0,"Interior"]
[null,32,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario Muro 1","Abr. Muro 1","Pesado",0.21,15,16,"Exterior"]
[null,32,null,"Muros","Ángulo Azimut","Orientación","Densidad Muro","Area (m²)","U [W/m²K]",null,"Puentes térmicos [ml]",null,null,null,"Posición Aislación",null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario Muro 2","Abr. Muro 2","Pesado",0.4,15,6,"Interior"]
[null,32,null,null,null,null,null,null,null,null,"P01","P02","P03",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario Muro 3","Abr. Muro 3","Pesado",0.5,15,1,"Interior"]
[null,32,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario Muro 4","Abr. Muro 4"]
[null,33,"Muro 1","Abr. Muro 1","0° ≤ Az < 22,5°","N","Pesado",20.571825392998065,0.21,null,null,null,null,null,"Exterior",null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario Muro 5","Abr. Muro 5"]
[null,34,"Muro 2","Muro Adiabatico","67,5° ≤ Az < 90°","E","Pesado",20.571825392998065,0,null,null,null,null,null,"Interior",null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario Muro 6","Abr. Muro 6"]
[null,35,"Muro 3","Abr. Muro 1","157,5° ≤ Az < 180°","S","Pesado",20.571825392998065,0.21,null,null,null,null,null,"Exterior",null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario Muro 7","Abr. Muro 7"]
[null,36,"Muro 4","Abr. Muro 1","-112,5° ≤ Az < -90°","O","Pesado",20.571825392998065,0.21,null,null,null,null,null,"Exterior",null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario Muro 8","Abr. Muro 8"]
[null,37,"Muro 5",null,"67,5° ≤ Az < 90°","E","",null,"",null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario Muro 9","Abr. Muro 9"]
[null,38,"Muro 6",null,"0° ≤ Az < 22,5°","N","",null,"",null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario Muro 10","Abr. Muro 10"]
[null,39,"Muro 7",null,"-112,5° ≤ Az < -90°","O","",null,"",null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario Muro 11","Abr. Muro 11"]
[null,40,"Muro 8",null,"67,5° ≤ Az < 90°","E","",null,"",null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario Muro 12","Abr. Muro 12"]
[null,41,"Muro 9",null,"67,5° ≤ Az < 90°","E","",null,"",null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario Muro 13","Abr. Muro 13"]
[null,42,"Muro 10",null,"0° ≤ Az < 22,5°","N","",null,"",null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario Muro 14","Abr. Muro 14"]
[null,43,"Muro 11",null,"67,5° ≤ Az < 90°","E","",null,"",null,null,null,null,null,""]
[null,44,"Muro 12",null,"67,5° ≤ Az < 90°","E","",null,"",null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,null,"Techos transmitancia"]
[null,45,"Muro 13",null,"67,5° ≤ Az < 90°","E","",null,"",null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,null,"Nombre","Abreviatura","U  [W/m2K]",null,"espesor techo solido [cm]","espesor aislante [cm]","Posición Aislación"]
[null,46,"Muro 14",null,"67,5° ≤ Az < 90°","E","",null,"",null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,null,"Adiabatico","Techo Adiabatico",0,null,15,null,"Interior"]
[null,47,"Muro 15",null,"67,5° ≤ Az < 90°","E","",null,"",null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario Techo 1","Abr. Techo 1",0.14000000000000001,null,null,28,"Exterior"]
[null,48,"Muro 16 + ..",null,"67,5° ≤ Az < 90°","E","",null,"",null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario Techo 2","Abr. Techo 2",0.24,null,null,14,"Interior"]
[null,48,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario Techo 3","Abr. Techo 3",0.47,null,null,8,"Interior"]
[null,48,null,"Puentes térmicos particulares"]
[null,48,null,"Alojada en el muro","Azimut","Orientación","Elemento perpendicular","Aislación ","Longitud [m]",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Pisos transmitancia"]
[null,48,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nombre","Abreviatura","U  Piso ventilado","Aislación bajo piso contacto terreno",null,"Refuerzo Aislación Vert. ",null,null,"Refuerzo Aislación horiz.",null,null,"Posición "]
[null,48,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"[W/m2K]","l [W/mK]","e aislante [cm]","l [W/mK]","e aislante [cm]","D [cm]","l [W/mK]","e aislante [cm]","D [cm]","Aislación"]
[null,49,"P04",null,"0° ≤ Az < 22,5°","N",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Adiabatico","Piso Adiabatico",0]
[null,50,"P04",null,"90° ≤ Az < 112,5°","E",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario Piso 1","Abr. Piso 1",0.21,0.04,15,0.04,10,60,null,null,null,"Exterior"]
[null,51,"P04",null,"0° ≤ Az < 22,5°","N",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario Piso 2","Abr. Piso 2",0.39,0.04,5,0.04,5,60,null,null,null,"Interior"]
[null,52,"P04",null,"0° ≤ Az < 22,5°","N",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Definido por usuario Piso 3","Abr. Piso 3",0.7,1.63,15,1.63,0,60,null,null,null,"Interior"]
[null,53,"P04",null,"0° ≤ Az < 22,5°","N"]
[null,53]
[null,53,null,"Tipo Puerta","Azimut","Orientación",null,"Categoría para Infiltraciones",null,null,"Alto [m]","Ancho [m]",null,"Área vidrio [m2]",null,"FAV 1",null,"FAV 2 Izquierda",null,"FAV 2 Derecha",null,"FAV 3"]
[null,53,null,null,null,null,null,null,null,null," (incluye marco)",null,null,null,null,"D","L","P","S","P","S","E","T","b","a"]
[null,53]
[null,54,"Puerta 1",null,"90° ≤ Az < 112,5°","E",null,"Madera Solida",null,null,null,null,null,0]
[null,55,"Puerta 2",null,null,0,null,"Madera Solida",null,null,null,null,null,0]
[null,56,"Puerta 3",null,"0° ≤ Az < 22,5°","N",null,null,null,null,null,null,null,0]
[null,56]
[null,56,null,"Tipo Ventana","Azimut","Orientación","Elemento envolvente donde se encuentra ","Tipo de Cierre de ventana","Posición Ventanal","Aislación Con/Sin retorno","Alto [m] (H)","Ancho [m] (W)","Categoría para PT y Infilt","Tipo",null,"FAV 1",null,"FAV 2 Izquierda",null,"FAV 2 Derecha",null,"FAV 3"]
[null,56,null,"Ventana (incluye marco)",null,null,null,null,null,null,null,null,"Marco",null,null,"D","L","P","S","P","S","E","T","b","a"]
[null,56]
[null,57,"Ventana 1","DVH con 12mm","67,5° ≤ Az < 90°","E","Abr. Muro 1","Corredera","Interior","Con",1.25,5,"PVC","Madera"]
[null,58,"Ventana 2","DVH con 12mm","0° ≤ Az < 22,5°","N","Abr. Muro 2","Corredera","Interior","Con",1.25,5,"PVC","Madera"]
[null,59,"Ventana 3","DVH con 12mm","-135° ≤ Az < -112,5°","SO","Abr. Muro 3","Corredera","Interior","Con",1.25,5,"PVC","Madera"]
[null,60,"Ventana 4","DVH con 12mm","-90° ≤ Az < -67,5°","O","Abr. Muro 4","Corredera","Interior","Con",1.25,5,"PVC","Madera"]
[null,61,"Ventana 5",null,null,0]
[null,62,"Ventana 6",null,null,0]
[null,63,"Ventana 7",null,null,0]
[null,64,"Ventana 8",null,null,0]
[null,65,"Ventana 9",null,null,0]
[null,66,"Ventana 10",null,null,0]
[null,67,"Ventana 11",null,null,0]
[null,68,"Ventana 12",null,null,0]
[null,69,"Ventana 13",null,null,0]
[null,70,"Ventana 14",null,null,0]
[null,71,"Ventana 15",null,null,0]
[null,72,"Ventana 16",null,null,0]
[null,73,"Ventana 17",null,null,0]
[null,74,"Ventana 18",null,null,0]
[null,75,"Ventana 19",null,null,0]
[null,76,"Ventana 20",null,null,0]
[]
[null,76,null,null,"% Anual referencial Rad Directa",null,null,1,null,"% Anual referencial Rad Directa",null,null,1,null,"% Anual referencial Rad Directa",null,null,1,null,"% Anual referencial Rad Directa",null,null,1]
[null,77,"Orientación",null,"N","Azimut","-22,5° ≤ Az < 0°",null,null,"E","Azimut","67,5° ≤ Az < 90°",null,null,"S","Azimut",null,null,null,"O","Azimut"]
[null,78,"Dimensiones",null,"División","A [m]","B [m]","D [m]",null,"División","A [m]","B [m]","D [m]",null,"División","A [m]","B [m]","D [m]",null,"División","A [m]","B [m]","D [m]"]
[null,79,"Obstrucción 1"]
[null,80,"Obstrucción 2"]
[null,81,"Obstrucción 3"]
[null,82,"Obstrucción 4"]
[null,83,"Obstrucción 5"]
[null,84,"Obstrucción 6"]
[null,85,"Obstrucción 7"]
[null,86,"Obstrucción 8"]
[]
[null,86,null,null,"% Anual referencial Rad Directa",null,null,1,null,"% Anual referencial Rad Directa",null,null,1,null,"% Anual referencial Rad Directa",null,null,1,null,"% Anual referencial Rad Directa",null,null,1]
[null,87,"Orientación",null,"NE","Azimut",null,null,null,"SE","Azimut",null,null,null,"SO","Azimut",null,null,null,"NO","Azimut"]
[null,88,"Dimensiones",null,"División","A [m]","B [m]","D [m]",null,"División","A [m]","B [m]","D [m]",null,"División","A [m]","B [m]","D [m]",null,"División","A [m]","B [m]","D [m]"]
[null,89,"Obstrucción 1"]
[null,90,"Obstrucción 2"]
[null,91,"Obstrucción 3"]
[null,92,"Obstrucción 4"]
[null,93,"Obstrucción 5"]
[null,94,"Obstrucción 6"]
[null,95,"Obstrucción 7"]
[null,96,"Obstrucción 8"]
[null,96]
[null,96,null,"Techos",null,"Densidad Techo","Area (m²)","U [W/m²K]",null,null,"Camaras de aire","Tipo de cubierta",null,"Posición Aislación"]
[null,96]
[null,97,"Techo 1","Abr. Techo 2",null,"Pesado",80,0.24,null,null,"Sin camara","Cubierta normal",null,"Interior"]
[null,98,"Techo 2",null,null,null,null,"",null,null,null,null,null,""]
[null,99,"Techo 3",null,null,null,null,"",null,null,null,null,null,""]
[null,100,"Techo 4",null,null,null,null,"",null,null,null,null,null,""]
[null,101,"Techo 5+..",null,null,null,null,"",null,null,null,null,null,""]
[null,101]
[null,101,null,"Pisos",null,"Densidad Piso","Area (m²)","U [W/m²K]",null,null,"Perímetro contacto terreno [m]","Piso ventilado",null,"Posición Aislación",null,null,null,"Ls [W/K]"]
[null,101]
[null,102,"Piso 1","Abr. Piso 1",null,"Pesado",80,0.21,null,null,null,"Ventilado",null,"Exterior",null,null,null,0]
[null,103,"Piso 2",null,null,null,null,"",null,null,null,"No Ventilado",null,"",null,null,null,0]
[null,104,"Piso 3",null,null,null,null,"",null,null,null,"No Ventilado",null,"",null,null,null,0]
[null,105,"Piso 4+..",null,null,null,null,"",null,null,null,"No Ventilado",null,"",null,null,null,0]
[null,105]
[null,105]
[null,105,null,"Resumen Envolvente "]
[null,105]
[null,105,null,"Elementos Opacos",null,null,null,"Elementos traslucidos",null,null,"Perdidas Puentes térmicos"]
[null,105,null,"Área total [m2]","Área Efectiva [m2]","U [W/Km²]",null,"Área [m2]","U [W/Km²]",null,"P01","P02","P03","P04","P05","Total",null,null,"U*A + jL [W/K]",null,"[m2] Envolvente no adiabatica"]
[null,105,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,246.71547617899421]
[null,106,"Horiz",80,80,0.24,null,0,0,null,null,null,null,null,null,null,null,"Techos",19.2]
[null,107,"N",21.821825392998065,1.2499999999999998,5.8,null,5,2.85,null,0,0,0,0,0.25,0.25,null,"N",21.75]
[null,108,"NE",0,0,0,null,0,0,null,0,0,0,0,0,0,null,"NE",0]
[null,109,"E",20.571825392998065,20.571825392998065,0.21,null,0,0,null,0,0,0,0,0,0,null,"E",4.3200833325295935]
[null,110,"SE",1.2499999999999998,1.2499999999999998,5.8,null,5,2.85,null,0,0,0,0,0.25,0.25,null,"SE",21.75]
[null,111,"S",21.821825392998065,21.821825392998065,0.53020694301046267,null,5,2.85,null,0,0,0,0,0,0,null,"S",25.820083332529592]
[null,112,"SO",0,0,0,null,0,0,null,0,0,0,0,0,0,null,"SO",0]
[null,113,"O",21.821825392998065,21.821825392998065,0.53020694301046267,null,5,2.85,null,0,0,0,0,0.25,0.25,null,"O",26.070083332529592]
[null,114,"NO",0,0,0,null,0,0,null,0,0,0,0,0,0,null,"NO",0]
[null,115,"Pisos ",80,80,0.21000000000000002,null,null,null,"Pisos Ls",null,null,null,null,null,0,null,"Pisos [ml]",16.8]
[null,115]
[null,115]
[null,115]
[null,115,null,"4.- Perfil de uso"]
[null,115]
[null,115,null,"4.1.- Condiciones de uso de la vivienda"]
[null,115]
[null,115,null,null,null,null,null,null,"Cargas internas [W/m2]"]
[null,115,null,null,null,null,null,null,"Enero","Febrero","Marzo","Abril","Mayo","Junio","Julio","Agosto","Septiembre","Octubre","Noviembre","Diciembre"]
[null,115,null,null,null,null,null,0,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996]
[null,115,null,null,null,null,null,1,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996]
[null,115,null,null,null,null,null,2,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996]
[null,115,null,null,"[W/m2]",null,null,3,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996]
[null,115,null,null,null,null,null,4,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996]
[null,115,null,null,"Diurna","Nocturna",null,5,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996]
[null,116,"Usuarios",null,4.92,4.0999999999999996,null,6,3.28,3.28,3.28,3.28,3.28,3.28,3.28,3.28,3.28,3.28,3.28,3.28]
[null,117,"Iluminación cuando luz natural < 250 Lux",null,1.5,0,135.36000000000001,7,3.9359999999999999,3.9359999999999999,3.9359999999999999,3.9359999999999999,5.4359999999999999,5.4359999999999999,5.4359999999999999,3.9359999999999999,3.9359999999999999,3.9359999999999999,3.9359999999999999,3.9359999999999999]
[null,117,null,null,null,null,null,8,1.968,1.968,1.968,1.968,1.968,1.968,1.968,1.968,1.968,1.968,1.968,1.968]
[null,117,null,null,null,null,null,9,1.23,1.23,1.23,1.23,1.23,1.23,1.23,1.23,1.23,1.23,1.23,1.23]
[null,117,null,null,null,null,null,10,1.23,1.23,1.23,1.23,1.23,1.23,1.23,1.23,1.23,1.23,1.23,1.23]
[null,117,null,null,null,null,null,11,1.23,1.23,1.23,1.23,1.23,1.23,1.23,1.23,1.23,1.23,1.23,1.23]
[null,117,null,null,null,null,null,12,1.23,1.23,1.23,1.23,1.23,1.23,1.23,1.23,1.23,1.23,1.23,1.23]
[null,117,null,null,null,null,null,13,1.23,1.23,1.23,1.23,1.23,1.23,1.23,1.23,1.23,1.23,1.23,1.23]
[null,117,null,null,null,null,null,14,1.23,1.23,1.23,1.23,1.23,1.23,1.23,1.23,1.23,1.23,1.23,1.23]
[null,117,null,null,null,null,null,15,1.23,1.23,1.23,1.23,1.23,1.23,1.23,1.23,1.23,1.23,1.23,1.23]
[null,117,null,null,null,null,null,16,1.476,1.476,1.476,1.476,1.476,1.476,1.476,1.476,1.476,1.476,1.476,1.476]
[null,117,null,null,null,null,null,17,2.46,2.46,2.46,2.46,2.46,2.46,2.46,2.46,2.46,2.46,2.46,2.46]
[null,117,null,null,null,null,null,18,2.46,2.46,2.46,2.46,2.46,3.96,3.96,2.46,2.46,2.46,2.46,2.46]
[null,117,null,null,null,null,null,19,3.69,3.69,5.1899999999999995,5.1899999999999995,5.1899999999999995,5.1899999999999995,5.1899999999999995,5.1899999999999995,5.1899999999999995,5.1899999999999995,3.69,3.69]
[null,117,null,null,null,null,null,20,5.9279999999999999,5.9279999999999999,5.9279999999999999,5.9279999999999999,5.9279999999999999,5.9279999999999999,5.9279999999999999,5.9279999999999999,5.9279999999999999,5.9279999999999999,5.9279999999999999,5.9279999999999999]
[null,117,null,null,null,null,null,21,6.42,6.42,6.42,6.42,6.42,6.42,6.42,6.42,6.42,6.42,6.42,6.42]
[null,117,null,null,null,null,null,22,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996]
[null,117,null,null,null,null,null,23,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996,4.0999999999999996]
[null,117]
[null,117,null,null,null,null,null,null,"Renovaciones de aire por hora [1/hr]"]
[null,117,null,null,null,null,null,null,"Enero","Febrero","Marzo","Abril","Mayo","Junio","Julio","Agosto","Septiembre","Octubre","Noviembre","Diciembre"]
[null,117,null,"Infiltraciones",null,null,null,0,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016]
[null,117,null,null,null,null,null,1,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016]
[null,118,"¿Cuenta con ensayo de presurización?",null,null,"No",null,2,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016]
[null,118,null,null,null,null,null,3,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016]
[null,119,"Indicar valor del ensayo de presurización",null,null,null,"[RAH] a 50Pa",4,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016]
[null,119,null,null,null,null,null,5,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016]
[null,120,"De existir ductos de ventilación, ¿Cuántos hay?",null,null,null," [un]",6,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016]
[null,120,null,null,null,null,null,7,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016]
[null,121,"De existir Celosías, ¿Cuántas hay?",null,null,null," [un]",8,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016]
[null,121,null,null,null,null,null,9,3.8262,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016]
[null,121,null,"Ventilación",null,null,null,10,3.8262,3.8262,3.8262,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,3.8262]
[null,121,null,null,null,null,null,11,3.8262,3.8262,3.8262,3.8262,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,3.8262,3.8262]
[null,122,"Ventilación Mecánica (VM)",null,"Extractor colectivo en edificio",null,null,12,3.8262,3.8262,3.8262,3.8262,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,3.8262,3.8262,3.8262]
[null,122,null,null,null,null,null,13,0.82620000000000016,3.8262,3.8262,3.8262,3.8262,0.82620000000000016,0.82620000000000016,0.82620000000000016,3.8262,3.8262,3.8262,3.8262]
[null,123,"Eficiencia Recuperador de Calor, si aplica ",null,null,null," [%]",14,0.82620000000000016,0.82620000000000016,3.8262,3.8262,3.8262,0.82620000000000016,0.82620000000000016,0.82620000000000016,3.8262,3.8262,3.8262,3.8262]
[null,123,null,"Eficiencia por defecto",null,50," [%]",15,3.8262,3.8262,3.8262,3.8262,3.8262,0.82620000000000016,0.82620000000000016,0.82620000000000016,3.8262,3.8262,3.8262,3.8262]
[null,123,null,null,null,null,null,16,3.8262,3.8262,3.8262,3.8262,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,3.8262,3.8262,3.8262]
[null,124,"¿Tiene Sensor de CO2?",null,null,"No",null,17,3.8262,3.8262,3.8262,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,3.8262,3.8262]
[null,124,null,null,null,null,null,18,3.8262,3.8262,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,3.8262]
[null,125,"De tener, RAH según Memoria de Cálculo",null,null,null,"[RAH]",19,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016]
[null,125,null,null,null,null,null,20,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016]
[null,125,null,null,null,null,null,21,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016]
[null,125,null,null,null,null,null,22,3.8262,3.8262,3.8262,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,3.8262]
[null,125,null,null,null,null,null,23,3.8262,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016,0.82620000000000016]
[null,125]

{"sheet":"Calculo","index":3,"n_rows":26,"n_cols":14,"rows_kept":26,"cut":false,"hidden":false,"merged":[]}
[]
[null,null,"Parámetros de operación",null,null,null,null,"DATOS RECINTO:"]
[]
[null,"Recup. de calor.","No","[ ]",null,null,"Elementos Opacos",null,null,null,"Elementos traslucidos",null,null,"Puentes térmicos"]
[null,"Eficiencia recup.",0,"[ ]",null,null,"Área total [m2]","Área Efectiva [m2]","U [W/Km²]",null,"Área [m2]","U [W/Km²]",null,"[W/K]"]
[null,"Sistema de clima.","No","[ ]"]
[]
[null,null,null,null,null,"TECHO",80,80,0.84,null,0,3.6]
[null,null,null,null,null,"NORTE:",21.821825392998065,1.2499999999999998,4,null,5,5.8,null,0.25]
[null,null,null,null,null,"NOR-ESTE:",0,0,0,null,0,0,null,0]
[null,null,null,null,null,"ESTE:",20.571825392998065,20.571825392998065,4,null,0,5.8,null,0]
[null,null,null,null,null,"SUR-ESTE:",1.2499999999999998,1.2499999999999998,4,null,5,5.8,null,0.25]
[null,null,null,null,null,"SUR:",21.821825392998065,21.821825392998065,4,null,5,5.8,null,0]
[null,null,null,null,null,"SUR-OESTE:",0,0,0,null,0,0,null,0]
[null,null,null,null,null,"OESTE:",21.821825392998065,21.821825392998065,4,null,5,5.8,null,0.25]
[null,null,null,null,null,"NOR-OESTE:",0,0,0,null,0,0,null,0]
[null,null,null,null,null,"PISO:",80,80,3.6,null,null,null,null,0]
[]
[]
[null,null,null,null,null,null,"Area [m²]","Altura [m]","Volumen [m3]"]
[]
[null,null,null,null,null,"Piso 1",80,2.5,200]
[null,null,null,null,null,"Piso 2",0,0,0]
[null,null,null,null,null,"Piso 3+4+..",0,0,0]
[]
[null,null,null,null,null,"Total ",80,null,200]

{"sheet":"Resultados","index":4,"n_rows":5,"n_cols":57,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
[{"$f":"+COUNTA(C6:C1048576)/25*26+6","v":6},"Fila a insertar datos (NO borrar)"]
[{"$f":"+Calculo!C23","v":0}]
[]
[null,null,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26,27,28,29,30,31,32,33,34]
[null,null,"Tiempo [hrs]","Tiempo [s]","Mes","T° exterior","Qsol_ef tot [W]","Qgen pers [W]","Qgen ilum [W]","Qgen equip [W]","TsolH","TsolN","TsolNE","TsolE","TsolSE","TsolS","TsolSO","TsolO","TsolNO","T Interior [°C]","Q Envolvente [W]","Q Piso_vent [W]","Q Ventanas [W]","Q Techo [W]","Q Muros [W]","Q Piso_terreno [W]","Q Ventilacion [W]","Q Recuperado [W]","Q Infiltraciones [W]","QClima [W]",null,"Q Masa_tot [W]","TmasaHOR [°C]","Q Masa_ad [W]","Demanda Calef. [Wh]","Demanda Ref. [Wh]","Qtot [W]","Q_techo_v [W]","Q_techo_opaco [W]","Q_norte_v [W]","Q_norte_opaco [W]","Q_noreste_v [W]","Q_noreste_opaco [W]","Q_este_v [W]","Q_este_opaco [W]","Q_sureste_v [W]","Q_sureste_opaco [W]","Q_sur_v [W]","Q_sur_opaco [W]","Q_suroeste_v [W]","Q_suroeste_opaco [W]","Q_oeste_v [W]","Q_oeste_opaco [W]","Q_noroeste_v [W]","Q_noroeste_opaco [W]","Q_piso_vent_SA [W]","Q_piso_terre_SA [W]"]